/Users/andrea/_magisterarbeit/korpus/clean/testkorpus/26/file17.html NN ----------------------------------------- : Cutting NP with IN the DT Water NP Jet NP Creating VVG Your PP$ Design NN Choose VV your PP$ design NN tool NN , , CorelDraw NP is VBZ an DT easy JJ one CD Create VVP your PP$ design NN , , and CC export VV it PP as IN a DT . SENT dxf NP file NN OMAX NP software NN Grab VVP the DT OMAX NP software NN from IN the DT NEMO NP computer NN on IN the DT windows NNS network NN Open VV up RP the DT OMAX NP shortcut NN it PP created VVD on IN your PP$ desktop NN Prepare VV Your PP$ Design NN For IN Cutting NP Use NP the DT File NP Open NP command NN to TO open VV your PP$ . SENT dxf NP file NN Set VVD the DT quality NN of IN cut NN you PP want VVP Right NP Click NP on IN the DT big JJ Q NP button NN , , select VVP all RB Choose VV your PP$ quality NN 1 CD is VBZ coarse JJ , , 5 CD is VBZ fine JJ , , 3 CD usually RB works VVZ fine RB Set VV up RP the DT traverses NNS needed VVN to TO make VV the DT cut NN Right NP Click NP on IN the DT Lead JJ I NN O NN button NN Select NP AutoPath NP Quick NP The DT green JJ lines NNS are VBP traverses NNS not RB cuts VVZ Set VV up RP the DT path NN for IN the DT jet NN Right NP Click NP on IN the DT Path NP button NN Select NP Automatically RB Generate VV Click NP at IN the DT start NN of IN a DT traverse NN , , where WRB you PP want VVP it PP to TO start VV It PP generates VVZ the DT path NN for IN your PP$ approval NN Check VV to TO make VV sure JJ it PP looks VVZ allright NN the DT path NN is VBZ the DT dark JJ red JJ line NN Hit VVP save VV to TO accept VV it PP Export NN the DT design NN Stick NP in IN a DT floppy JJ Select NP File NP Transfer NN Path NN and CC Drawing VVG to TO 3 CD . SENT 5 CD Floppy JJ Prepare VVP the DT Pump NP to TO Use VV It PP will MD probably RB be VB on IN , , if IN not RB , , turn VV the DT big JJ switch NN on IN the DT right NN of IN the DT computer NN housing NN to TO the DT On NP position NN Rotate VV the DT switch NN on IN the DT left NN of IN the DT pump NN to TO the DT left NN of IN the DT computer NN housing NN twice RB Place VV your PP$ material NN on IN the DT bed NN and CC clamp VV or CC weight VV it PP down RB Check VV the DT abrasive NN to TO make VV sure JJ it PP is VBZ at IN least JJS half RB full RB Check VV the DT abrasive JJ feeding NN tube NN to TO make VV sure JJ it PP is VBZ clear JJ Set VV up RP Your PP$ Design NN for IN Cutting NP Lift VV the DT cover NN and CC insert VV your PP$ diskette NN Click NP the DT Make NP button NN Hit VVP open VV and CC select VV the DT . SENT ORD JJ file NN from IN your PP$ diskette NN Enter NP the DT appropriate JJ machinability NN rating NN and CC thickness NN Set VVN Up IN the DT Cutter NP For IN Your PP$ Design NN Use VV the DT arrows NNS to TO move VV the DT head NN till IN you PP are VBP at IN your PP$ zero CD point NN Click NP the DT Set VVN UZ NP button NN to TO set VV the DT coordinate VV zero CD point NN Set VVN up RP the DT nozzle NN Tighten VV down RP the DT main JJ nozzle NN till IN it PP locks VVZ using VVG the DT winder NN on IN top NN Keep VV going VVG till IN it PP makes VVZ contact NN Turn VV it PP back VV half PDT a DT turn NN Lock NP down RB the DT handle VV on IN the DT side NN Cut VV It PP Hit VVP the DT begin VVP button NN Hit VVP run VVP once RB Raise VV the DT H NP 2 CD O NN till IN about RB 1 CD 2 CD inch NN above IN your PP$ material NN Hit VVP the DT start NN button NN The DT space NN bar NN will MD pause VV your PP$ design NN