/Users/andrea/_magisterarbeit/korpus/clean/trainkorpus/29/file_184.html NN ----------------------------------------- : COLLISION NN INDUSTRY NN CONFERENCE NN Glossary NN of IN Terms NNS This DT document NN was VBD originally RB published VVN in IN January NP 1997 CD and CC is VBZ currently RB being VBG updated VVN . SENT If IN you PP notice VVP missing JJ terms NNS or CC have VHP suggestions NNS or CC corrections NNS for IN the DT definitions NNS of IN existing JJ terms NNS , , contact NN one NN of IN the DT Co NP Chairs NNS listed VVN below IN . SENT Sharon NP Kellum NP , , Co NP ChairUnited NP Recyclers NNS Groupph NP . SENT 303 CD 367 CD 4391 CD Click NP here RB to TO download VV complete JJ document NN in IN MS NN Word NP . SENT Return NN to TO Home NP Page NP General NP Automotive NP Terms NNS Unibody NP Terms NNS Insurance NP Terms NNS Computer NP Estimating VVG Terms NNS Time NP Terms NNS General NP Automotive NP Terms NNS A DT B NP C NP D NP E NP F NP G NP H NP I NP J NP L NP M NP N NP O NP P NN Q NP R NP S NP T NN U NP V NN W NP X NP Z NP A NP Back RB to TO Top JJ ABRASIVE NN . SENT Substance NN used VVD to TO wear VV away RP a DT surface NN by IN friction NN . SENT ABRASIVE JJ COATING NN . SENT In IN closed JJ coat NN paper NN , , the DT adhesive NN is VBZ completely RB coated JJ with IN abrasive NN , , and CC in IN open JJ coat NN paper NN , , the DT adhesive NN is VBZ partially RB exposed VVN , , for IN the DT abrasive NN is VBZ not RB put VVN on IN the DT paper NN close NN together RB . SENT ACCUMULATOR NN . SENT Assembly NN that IN acts NNS as IN a DT refrigerator NN storage NN container NN to TO receive VV liquid JJ , , vapor NN , , and CC refrigerant JJ oil NN from IN the DT evaporator NN . SENT ACETYLENE NN . SENT Gas NN used VVD for IN oxyacetylene NN welding VVG . SENT ACID JJ CORE NN . SENT Solder NN in IN a DT tubular JJ wire NN form NN in IN which WDT the DT interior NN contains VVZ a DT flux NN . SENT ACRYLIC JJ RESINS NNS . SENT Synthetic JJ resin NN that WDT has VHZ excellent JJ color NN retention NN and CC clarity NN and CC that WDT is VBZ used VVN in IN both DT lacquer NN and CC enamel NN . SENT ACTIVATOR NN . SENT Additive NN used VVD to TO speed VV up RP the DT curing VVG of IN paint NN resins NNS . SENT ALTERNATOR NN . SENT Device NN on IN a DT vehicle NN that IN when WRB turned VVD produces VVZ electricity NN ALUMINUM NN OXIDE NN . SENT Sharp JJ and CC hard JJ abrasive NN that WDT is VBZ made VVN by IN fusing VVG mineral NN bauxite NN at IN high JJ temperatures NNS . SENT AMBIENT JJ TEMPERATURE NN . SENT Temperature NN of IN the DT air NN surrounding VVG an DT object NN . SENT ANTICORROSIVE JJ . SENT Materials NNS applied VVD to TO metal NN to TO give VV corrosion NN resistance NN . SENT ANTICORROSIVE JJ AND CC INHIBITOR NN . SENT Protective JJ coatings NNS applied VVN on IN metal NN surfaces VVZ to TO retard VV or CC prevent VV corrosion NN and CC said VVD to TO be VB anticorrosive JJ or CC corrosion NN inhibitive JJ . SENT ARMREST NN . SENT Part NN of IN the DT door NN trim VV on IN which WDT the DT arm NN may MD be VB rested VVD . SENT ASSEMBLY NN . SENT A DT number NN of IN auto NN body NN parts NNS that WDT are VBP either RB bolted VVN or CC welded VVN together RB forming VVG a DT single JJ unit NN . SENT ATOMIZATION NN . SENT Breaking VVG up RP a DT fluid NN with IN an DT air NN stream NN , , such JJ as IN with IN a DT spray NN gun NN . SENT ATOMIZE VV . SENT Air NN at IN the DT gun NN nozzle NN breaks VVZ up RP the DT paint NN and CC solvents NNS into IN fine JJ particles NNS . SENT AUTOMATIC JJ LOAD NN LEVELING VVG SYSTEM NN . SENT System NN used VVD on IN some DT vehicles NNS to TO raise VV the DT vehicle NN to TO counteract VV the DT weight NN of IN the DT passengers NNS . SENT AUTOMATIC JJ PRESSURE NN SWITCH NN . SENT Used VVN on IN a DT compressor NN to TO release VV the DT air NN pressure NN in IN the DT cylinders NNS . SENT B SYM Back RB to TO General NP Terms NNS Index NN BACK RB SANDING VVG . SENT Technique NN of IN sanding VVG a DT surface NN to TO taper VV the DT paint NN film NN away RB from IN the DT metal NN repaired VVN area NN . SENT BACKFIRE VV . SENT Malfunctioning VVG of IN a DT torch NN , , causing VVG the DT flame NN to TO go VV out RP with IN a DT loud JJ snap NN or CC pop NN . SENT BACKHAND RB WELDING VVG . SENT When WRB the DT torch NN , , in IN the DT case NN of IN a DT right JJ hand NN operator NN , , is VBZ moved VVN in IN the DT opposite JJ way NN from IN left VVN to TO right RB instead RB of IN right NN to TO left VVN as RB in IN the DT usual JJ practice NN . SENT BAFFLE VV . SENT Part NN used VVD in IN a DT spray NN gun NN to TO divert VV the DT air NN stream NN . SENT Also RB a DT part NN of IN the DT radiator NN support NN on IN some DT cars NNS . SENT BAKING VVG . SENT Application NN of IN heat NN to TO cure VV and CC dry VV a DT coating NN . SENT In IN automotive JJ refinishing VVG , , baking VVG is VBZ used VVN to TO speed VV up RP the DT drying VVG of IN air NN drying VVG lacquers NNS and CC enamel NN and CC is VBZ sometimes RB called VVN force NN drying VVG . SENT The DT metal NN temperature NN in IN refinish NNS baking VVG usually RB does VVZ not RB exceed VV 180 CD F NN 82 CD . SENT 2 CD C NP . SENT BANDING VVG . SENT Single JJ coat NN of IN paint NN applied VVN to TO frame VV in IN an DT area NN to TO be VB sprayed VVN . SENT BASECOAT NP CLEARCOAT NP . SENT Type NN of IN paint NN coating NN . SENT BATTERY NN . SENT Part NN used VVN in IN vehicles NNS to TO store VV electrical JJ energy NN used VVN to TO start VV the DT vehicle NN . SENT BETTERMENT NN FACTOR NN . SENT Term NN used VVD in IN the DT insurance NN industry NN when WRB a DT part NN such JJ as IN a DT tire NN is VBZ replaced VVN , , and CC the DT insurance NN company NN pays VVZ for IN the DT unworn JJ part NN and CC the DT customer NN pays VVZ for IN the DT amount NN that WDT was VBD worn VVN . SENT BINDER NN . SENT Resin NN used VVD to TO hold VV the DT pigment NN in IN a DT paint NN film NN . SENT BLEEDING VVG . SENT Action NN whereby WRB the DT color NN of IN a DT stain NN or CC other JJ material NN works VVZ up RP into IN succeeding VVG coats NNS and CC imparts VVZ a DT certain JJ amount NN of IN color NN . SENT This DT is VBZ characteristic JJ of IN certain JJ red JJ pigments NNS used VVN in IN lacquers NNS and CC enamels NNS . SENT A DT nonbleeding NN color NN is VBZ one NN that WDT is VBZ not RB soluble JJ in IN materials NNS used VVN over IN it PP and CC , , consequently RB , , does VVZ not RB work VV up RP into IN succeeding VVG coats NNS . SENT Bad JJ body NN filler NN will MD also RB cause VV bleeding NN . SENT BLENDING VVG . SENT Mixing VVG together RB of IN two CD or CC more JJR materials NNS or CC the DT gradual JJ shading NN of IN paint NN from IN one CD panel NN to TO the DT next JJ to TO assure VV color NN consistency NN . SENT BLISTERING VVG . SENT Bubbling VVG up RP of IN the DT paint NN film NN in IN the DT form NN of IN small JJ blisters NNS . SENT BLUSHING VVG . SENT White NP or CC grayish JJ cast NN that WDT sometimes RB forms VVZ on IN a DT lacquer NN film NN as IN it PP dries VVZ , , particularly RB under IN conditions NNS of IN hot JJ , , humid JJ weather NN . SENT BODY NN FILES NNS . SENT Variety NN of IN files NNS used VVN in IN accurately RB locating VVG surface NN irregularities NNS high JJ and CC low JJ spots NNS on IN damaged JJ areas NNS after IN they PP have VHP been VBN bumped VVN out RP . SENT Also RB used VVN in IN trimming VVG down RP solder NN and CC plastic JJ filled VVN areas NNS . SENT BODY NN SOLDER NN . SENT Alloy NN of IN tin NN and CC lead NN . SENT Its PP$ properties NNS may MD vary VV but CC the DT most RBS common JJ mixture NN consists VVZ of IN 30 CD tin NN and CC 70 CD lead NN or CC 30 CD 70 CD solder NN as IN it PP is VBZ usually RB called VVN . SENT BODY NN STRAPS NNS . SENT Specially RB designed VVN straps NNS made VVN out RP of IN strong JJ vulcanized VVD belting VVG material NN equipped VVN with IN wide JJ hooks NNS that WDT snugly RB fit VVP around IN the DT flanges NNS of IN various JJ body NN panels NNS . SENT They PP are VBP used VVN in IN repositioning VVG and CC pulling VVG different JJ assemblies NNS and CC parts NNS closer RBR together RB . SENT BODYING VVG . SENT Thickening VVG in IN the DT package NN , , usually RB due JJ to TO evaporation NN of IN solvents NNS or CC volatile JJ material NN because IN of IN excessive JJ heat NN or CC exposure NN to TO air VV during IN storage NN . SENT BOILING VVG POINT NN . SENT Temperature NN at IN which WDT the DT vapor NN pressure NN of IN a DT liquid NN exceeds VVZ the DT atmospheric JJ pressure NN and CC the DT liquid NN begins VVZ to TO boil VV . SENT BONDING VVG STRIPS NNS . SENT Narrow JJ strips NNS of IN laminated VVN fiberglass NNS bonded VVN to TO the DT inner JJ surface NN of IN the DT replacement NN panel NN and CC the DT adjoining JJ body NN panels NNS . SENT When WRB properly RB installed VVN , , the DT strips VVZ greatly RB strengthen VV the DT joint JJ and CC make VV alignment NN of IN the DT replacement NN panel NN with IN the DT rest NN of IN the DT body NN panels NNS much RB easier JJR . SENT BRAKE NN SYSTEM NN . SENT Hydraulic JJ system NN of IN levers NNS , , cylinders NNS , , surfaces VVZ and CC fluid NN used VVN to TO stop VV or CC slow VV down RP a DT vehicle NN . SENT BRAZE VV WELDING VVG . SENT When WRB bronze NN welding VVG rod NN in IN a DT molten JJ stage NN is VBZ deposited VVN on IN metals NNS that WDT are VBP heated VVN to TO a DT cherry JJ red NN . SENT similar JJ and CC dissimilar JJ metals NNS are VBP bonded VVN together RB . SENT BRIDGING VVG . SENT Ability NN of IN an DT enamel NN or CC lacquer NN to TO cover VV a DT crack NN , , void NN , , or CC other JJ small JJ gap NN . SENT BUBBLES NNS , , BLISTERS NNS AND CC BULGES NNS . SENT Damage NN that WDT occurs VVZ on IN vinyl NN roof NN covers VVZ . SENT BUFFING VVG . SENT Technique NN used VVD to TO polish VV an DT area NN to TO remove VV sanding VVG marks NNS of IN surface NN imperfections NNS . SENT BUFFING VVG COMPOUND NN . SENT Soft JJ paste NN containing VVG fine JJ abrasive NN in IN a DT neutral JJ medium NN , , used VVN to TO eliminate VV fine JJ scratches NNS and CC polish VV the DT topcoat NN . SENT BULL'S NP EYE NN . SENT Edge NN of IN a DT repaired VVN area NN of IN a DT paint NN film NN that WDT shows VVZ up RP after IN a DT surface NN has VHZ been VBN repainted VVN . SENT BURNING NN . SENT Condition NN resulting VVG from IN rubbing VVG a DT topcoat NN too RB hard RB . SENT The DT heat NN generated VVN by IN the DT friction NN of IN the DT rubbing NN pad NN may MD soften VV the DT surface NN and CC cause VV it PP to TO stick VV to TO the DT pad NN , , thus RB permanently RB marring VVG the DT finish NN . SENT BUTT NN WELD NN . SENT Two CD pieces NNS of IN similar JJ metal NN are VBP aligned VVN closely RB edge NN to TO edge VV . SENT The DT edges NNS are VBP tack NN welded VVN first RB and CC then RB by IN running VVG a DT good JJ bead NN are VBP solidly RB fused VVN together RB . SENT C SYM Back RB to TO General NP Terms NNS Index NP CAKING VVG . SENT Gathering VVG of IN sanding VVG dust NN into IN solid JJ cakes NNS sticking VVG to TO sandpaper NN . SENT Compare VV Gumming VVG CALCIUM NN CARBIDE NN . SENT Chemical NP used VVD to TO make VV acetylene NN gas NN . SENT CALIPER NN . SENT Part NN of IN the DT disk NN brake NN mechanism NN that WDT holds VVZ the DT brake NN pads VVZ . SENT CAMBER NN . SENT Inward RB or CC outward RB tilt VV of IN the DT wheel NN at IN the DT top NN . SENT It PP is VBZ the DT tire NN wearing VVG angle NN measured VVN in IN degrees NNS and CC is VBZ the DT amount NN the DT centerline NN of IN the DT wheel NN is VBZ tilted VVN from IN true JJ vertical JJ . SENT CARBON NN DIOXIDE NN . SENT Gas NN that WDT can MD be VB used VVN for IN MIG NP welding VVG . SENT CARBURIZING VVG FLAME NN . SENT Used VVN mostly RB for IN heating NN parts NNS and CC for IN soldering VVG . SENT It PP burns VVZ more JJR acetylene NN than IN oxygen NN through IN the DT torch NN . SENT Its PP$ inner JJ core NN is VBZ whitish JJ in IN color NN and CC has VHZ a DT feather NN . SENT Sometimes RB also RB called VVN a DT reducing VVG flame NN . SENT CASE NN HARDENING NN . SENT Surface NN coating NN that WDT will MD dry VV hard RB on IN top NN and CC remain VV more RBR or CC less RBR soft JJ underneath IN . SENT Compare VV Lifting NN . SENT CAST NN . SENT Tendency NN of IN one CD color NN to TO look VV like IN another DT . SENT CASTER NN . SENT Backward RB or CC forward RB tilt VV of IN the DT king NN pin NN or CC spindle NN support NN arm NN at IN the DT top NN . SENT It PP is VBZ the DT directional JJ control NN angle NN measured VVN in IN degrees NNS and CC is VBZ the DT amount NN the DT centerline NN of IN the DT spindle NN support NN arm NN is VBZ tilted VVN from IN the DT true JJ vertical JJ . SENT CATALYST NN . SENT Substance NN that WDT causes VVZ or CC speeds VVZ up RP a DT chemical NN reaction NN when WRB it PP is VBZ mixed VVN with IN another DT substance NN and CC that WDT does VVZ not RB change VV by IN itself PP . SENT CAULKING VVG COMPOUND NN . SENT Semi NN or CC slow JJ drying VVG plastic NN material NN used VVN to TO fill VV crevices NNS or CC seal NN joints NNS . SENT CENTER NN PLANE NN OR CC CENTERLINE NP . SENT Line NN in IN the DT center NN of IN vehicle NN from IN which WDT all DT side NN measurements NNS are VBP taken VVN . SENT CENTRIFUGAL JJ PRESSURE NN SWITCH NN . SENT Switch NN used VVD on IN a DT compressor NN to TO release VV the DT pressure NN in IN the DT cylinder NN . SENT CHALKING VVG . SENT Formation NN of IN soft JJ white JJ powder NN on IN the DT surface NN of IN a DT finish NN , , which WDT may MD be VB removed VVN by IN friction NN of IN the DT finger NN or CC similar JJ methods NNS . SENT CHECKING NN . SENT Small JJ , , irregular JJ cracks NNS going VVG partly RB or CC completely RB through IN a DT paint NN film NN . SENT Like IN alligatoring NN , , only RB very RB fine JJ cracks NNS . SENT Compare VV Cracking VVG and CC Crazing VVG . SENT CHEMICAL NN STAINING VVG . SENT Spotty JJ staining VVG or CC discoloration NN of IN the DT paint NN topcoat NN caused VVN by IN atmospheric JJ conditions NNS acid NN rain NN , , tree NN sap NN , , etc FW . SENT . SENT CHIPPING VVG . SENT Condition NN of IN the DT finish NN flaking VVG off RP or CC chipping VVG away RB from IN the DT surface NN underneath IN . SENT CHIPPING VVG HAMMER NN . SENT Special JJ hammer NN used VVN in IN removing VVG slag NN deposits NNS from IN a DT weld NN so RB that IN it PP can MD be VB inspected VVN for IN quality NN . SENT CHROMA NN . SENT Quality NN of IN a DT color NN that WDT combines VVZ hue NN and CC saturation NN . SENT CLEAN VV . SENT Opposite JJ of IN dirty JJ . SENT Describes VVZ a DT color NN with IN a DT bright JJ appearance NN rather RB than IN one CD that WDT has VHZ a DT drab JJ appearance NN . SENT The DT exclusion NN of IN black NN makes VVZ colors NNS cleaner JJR . SENT CLEAR JJ . SENT A DT coating NN of IN paint NN that WDT has VHZ no DT color NN . SENT CLEAR JJ COAT NN . SENT A DT clear JJ , , shiny JJ coat NN of IN paint NN e NN . SENT g NN . SENT urethane NN or CC acrylic JJ enamel NN applied VVN over IN the DT base NN or CC color NN coat NN of IN paint NN on IN a DT vehicle NN . SENT CLIP NN . SENT A DT group NN of IN related JJ vehicle NN parts NNS purchased VVN from IN a DT salvage NN yard NN as IN an DT assembly NN usually RB the DT complete JJ front NN or CC complete JJ rear JJ section NN of IN a DT vehicle NN . SENT Also RB known VVN as IN Salvage NP Clip NN . SENT CLOSED JJ COAT NN DISK NN . SENT Disk NN on IN which WDT the DT abrasive JJ grains NNS are VBP very RB densely RB spaced VVN . SENT Used VVN in IN disk NN sanding VVG and CC polishing VVG repaired VVN sheet NN metal NN . SENT COAT NN DOUBLE RB . SENT Two CD single JJ coats NNS applied VVD one CD after IN the DT other JJ with IN little JJ or CC no RB flash VV off RP time NN for IN the DT first JJ coat NN . SENT COAT NN SINGLE JJ . SENT Coat NN produced VVD by IN two CD passes NNS of IN a DT spray NN gun NN when WRB one PP pass VVP overlaps VVZ the DT other JJ 50 CD percent NN or CC by IN half NN steps NNS . SENT COLD JJ CRACKING VVG . SENT Cracking VVG of IN a DT paint NN job NN resulting VVG from IN a DT sudden JJ drop NN of IN temperature NN . SENT COLD JJ RAZOR NN KNIFE NN . SENT Knife NP used VVD to TO cut VV the DT adhesive NN of IN windshields NNS and CC backlites NNS . SENT COLLAPSED VVD HINGE VV BUCKLE NN . SENT Formed VVN whenever WRB a DT simple JJ hinge NN buckle NN extends VVZ and CC crosses VVZ over IN a DT stamped VVN in IN reinforcing VVG flange NN , , head NN , , or CC ridge NN on IN a DT flat JJ or CC reverse RB curved VVD concave JJ surface NN of IN an DT auto NN body NN panel NN . SENT Will MD also RB form VV when WRB box NN constructed VVN members NNS and CC a DT COLLAPSED JJ ROLLED JJ BUCKLE NN . SENT Formed VVN whenever WRB a DT hinge NN buckle NN extends VVZ or CC crosses VVZ over RP into IN the DT crowned VVN surface NN of IN a DT panel NN causing VVG the DT metal NN to TO collapse VV and CC shrink VV severely RB and CC a DT general JJ shortening NN up RB in IN the DT overall JJ length NN of IN the DT panel NN to TO occur VV . SENT COLOR NN COAT NN . SENT The DT single JJ stage NN or CC BASECOAT NN that WDT provides VVZ the DT final JJ color NN of IN a DT coating NN system NN . SENT COLOR NN RETENTION NN . SENT When WRB a DT color NN is VBZ exposed VVN to TO the DT elements NNS and CC does VVZ not RB change VV is VBZ said VVN to TO have VH good JJ color NN retention NN . SENT COMPARTMENT NN . SENT Separate JJ enclosure NN or CC section NN , , such JJ as IN the DT engine NN , , passenger NN and CC luggage NN compartment NN , , in IN an DT autobody NN . SENT COMPATIBILITY NN . SENT Ability NN of IN two CD or CC more JJR materials NNS to TO blend VV into IN a DT homogeneous JJ mixture NN and CC upon IN drying VVG , , a DT homogeneous JJ film NN without IN a DT subsequent JJ negative JJ chemical NN reaction NN . SENT COMPOUNDING NN . SENT Use NN of IN an DT abrasive NN either CC by IN hand NN or CC machine NN to TO smooth VV out RP and CC bring VV up RP the DT gloss VVP of IN an DT applied VVN topcoat NN . SENT COMPREHENSIVE JJ COVERAGE NN . SENT Term NN used VVD to TO describe VV a DT type NN of IN insurance NN protection NN designed VVN to TO cover VV loss NN from IN accidental JJ damage NN caused VVN by IN other JJ than IN collision NN . SENT COMPRESSOR NN . SENT Machine NN used VVD to TO compress VV air NN from IN atmospheric JJ pressure NN to TO a DT high JJ pressure NN . SENT CONDUCTOR NN . SENT Material NN such JJ as IN an DT electric JJ wire NN through IN which WDT electricity NN flows NNS . SENT CONE NN MANDREL NN . SENT Special JJ attachment NN used VVN with IN an DT abrasive JJ cone NN in IN sanding VVG hard RB to TO get VV at IN concave JJ surfaces VVZ around IN headlights NNS , , fender NN flanges NNS and CC trim JJ moldings NNS . SENT CONNECTORS NNS MALE JJ AND CC FEMALE JJ . SENT Attachments NNS used VVN in IN coupling NN two CD or CC more JJR extension NN tubes NNS together RB and CC to TO the DT various JJ rams NNS . SENT CONSTANT JJ VELOCITY NN JOINT NN . SENT Type NN of IN joint NN that WDT provides VVZ constant JJ , , even RB transfer VV of IN power NN . SENT CONTACT NN TIP NN . SENT Part NN of IN the DT MIG NP gun NN through IN which WDT the DT welding VVG rod NN moves NNS . SENT CONTAMINANTS NNS . SENT Any DT polish NN , , wax NN , , tree NN sap NN , , tar NN , , oil NN , , and CC the DT like IN that WDT would MD damage VV the DT paint NN film NN or CC spoil VV the DT adhesion NN of IN a DT new JJ paint NN film NN . SENT CONTRACTION NN . SENT Area NN that WDT reduces VVZ in IN size NN . SENT CONTROL NN POINTS NNS . SENT Areas NNS in IN the DT vehicle NN body NN that WDT are VBP used VVN to TO measure VV for IN dimensions NNS or CC to TO correct VV damage NN . SENT CONTROLLED VVN HEAT NN . SENT Heat NN from IN an DT acetylene NN torch NN that WDT is VBZ usually RB controlled VVN by IN the DT operator NN . SENT CONVENTIONAL JJ BODY NN CONSTRUCTION NN . SENT Type NN of IN construction NN where WRB the DT body NN and CC frame NN are VBP two CD entirely RB separate JJ units NNS held VVN together RB at IN various JJ points NNS by IN means NNS of IN body NN bolts NNS . SENT CONVERSION NN COATING NN . SENT Part NN of IN a DT metal NN treatment NN system NN that WDT modifies VVZ a DT metal NN substrate NN to TO increase VV adhesion NN and CC corrosion NN protection NN . SENT COOLING VVG SYSTEM NN . SENT System NN of IN parts NNS and CC fluid NN used VVN to TO cool VV the DT engine NN . SENT CORRECTIVE JJ PULL NN . SENT Application NN of IN force NN to TO remove VV collision NN damage NN . SENT CORROSION NN . SENT Chemical JJ reaction NN of IN oxygen NN and CC moisture NN , , or CC corrosive JJ materials NNS on IN a DT metal NN surface NN . SENT Usually RB referred VVN to TO as IN rusting VVG or CC oxidation NN . SENT CORROSION NN RESISTANT NN . SENT Material NN that WDT resists VVZ the DT effects NNS of IN corrosion NN . SENT COUPLER NN . SENT Permits VVZ the DT removal NN of IN the DT coupler NN tube NN without IN the DT loss NN of IN hydraulic JJ fluid NN from IN the DT ram NN making VVG it PP possible JJ to TO use VV the DT same JJ pump NN with IN a DT variety NN of IN rams NNS and CC spreaders NNS . SENT COVERAGE NN . SENT Quality NN some DT colors NNS have VHP to TO cover VV other JJ colors NNS and CC the DT area NN a DT certain JJ quantity NN of IN paint NN will MD cover VV . SENT COWL NN . SENT Front JJ part NN of IN the DT vehicle NN passenger NN compartment NN . SENT CRACKING VVG . SENT Crevices NNS or CC ruptures NNS going VVG completely RB through IN a DT film NN . SENT This DT is VBZ in IN contrast NN to TO alligatoring NN or CC checking NN where WRB crevices NNS slowly RB work VVP their PP$ way NN down RB from IN the DT surface NN . SENT CRATERING VVG . SENT Surface NN blemishes NNS in IN a DT freshly RB painted VVN surface NN , , usually RB in IN the DT form NN of IN small JJ round NN patches NNS also RB called VVN fisheyes NNS , , usually RB due JJ to TO contamination NN . SENT CRAWLING VVG . SENT Action NN of IN a DT finishing JJ material NN when WRB it PP appears VVZ to TO creep VV or CC crawl VV away RP from IN certain JJ spots NNS and CC leaves VVZ them PP uncoated JJ . SENT CRAZING VVG . SENT Very RB fine JJ minute NN cracks NNS on IN the DT surface NN that WDT is VBZ usually RB interlaced VVN . SENT CRISSCROSS JJ SEQUENCE NN . SENT Method NN of IN tightening VVG fasteners NNS by IN using VVG a DT system NN of IN tightening VVG in IN a DT side NN pattern NN across IN an DT opposite NN of IN last JJ fastener NN tightened VVD . SENT CROSS NN COAT NN . SENT Technique NN used VVD when WRB grinding VVG metal NN to TO remove VV deep JJ scratches NNS by IN grinding VVG the DT surface NN at IN a DT 90 CD degree NN angle NN . SENT CROSS NN DRAFT NN BOOTH NN . SENT Spray NN booth NN in IN which WDT the DT air NN flows VVZ from IN the DT rear JJ section NN to TO the DT front JJ section NN and CC is VBZ exhausted VVN . SENT CROSS NN TUBES NNS . SENT Tubes NNS of IN iron NN used VVN with IN specially RB designed VVN safety NN stand VVP to TO support VV a DT vehicle NN . SENT CROWN NN . SENT Term NN used VVD to TO describe VV the DT high JJ part NN of IN a DT round NN surface NN of IN a DT panel NN . SENT CRUSH NN ZONE NN . SENT Part NN designed VVN to TO bend VV or CC crush VV when WRB involved VVN in IN a DT collision NN . SENT CURING VVG . SENT Term NN used VVD to TO explain VV the DT hardening VVG process NN of IN paint NN or CC resins NNS . SENT CUT VV . SENT Cut VVN as IN applied VVN to TO surface VV coating NN denotes VVZ both CC the DT dissolving VVG of IN solid JJ material NN in IN a DT solvent JJ and CC the DT reducing VVG of IN the DT viscosity NN of IN liquid NN by IN the DT addition NN of IN a DT thinner JJR . SENT Can MD also RB refer VV to TO sanding VVG down RP a DT film NN as IN in IN cut NN and CC polish NN . SENT CUTS NNS , , SCUFFS NNS , , AND CC GOUGES VVZ . SENT Types NNS of IN damage NN that WDT occur VVP on IN vinyl NN roof NN covers VVZ . SENT CUTTING VVG TIP NN . SENT Attachment NN inserted VVN in IN an DT oxyacetylene NN torch NN to TO cut VV metal NN with IN the DT flame NN . SENT D SYM Back RB to TO General NP Terms NNS Index NP DARKEN VV . SENT By IN eliminating VVG white JJ , , solid JJ colors NNS become VVP darker JJR . SENT eliminating VVG metallic JJ flake NN makes VVZ metallic JJ colors NNS darker JJR . SENT DATA NN SHEETS NNS . SENT Sheets NNS that WDT contain VVP the DT required VVN measurements NNS for IN straightening VVG the DT frame NN or CC body NN to TO specifications NNS . SENT DATUM NN LINE NN . SENT Imaginary JJ line NN that WDT appears VVZ on IN frame NN blueprints NNS or CC charts NNS to TO help VV determine VV correct JJ frame NN height NN . SENT DEDICATED JJ BENCH NN . SENT Type NN of IN frame NN repair NN equipment NN using VVG jigs NNS to TO align VV a DT unibody NN vehicle NN . SENT DEFLECTOR NN UNIT NN . SENT Unit NN used VVD on IN a DT rail NN to TO deflect VV the DT laser NN beam NN . SENT DIAMOND NN . SENT Frame NN misalignment NN resulting VVG from IN a DT heavy JJ impact NN on IN the DT corner NN of IN either DT side NN rail NN of IN the DT frame NN that WDT is VBZ sufficient JJ to TO push VV the DT side NN rail NN back RB . SENT As IN a DT result NN the DT cross NN members NNS are VBP pushed VVN out RP of IN a DT right JJ angle NN with IN the DT side NN rail NN . SENT DILUTANTS NNS . SENT Volatile JJ liquids NNS that WDT are VBP not RB solvent JJ for IN nitrocellulose NN . SENT They PP are VBP used VVN in IN nitrocellulose NN lacquer NN to TO lower JJR viscosity NN and CC give VV certain JJ other JJ properties NNS . SENT DINGING VVG . SENT Reshaping VVG and CC leveling VVG out RP of IN damaged JJ metal NN by IN means NNS of IN on IN and CC off IN the DT dolly NN hammering VVG after IN the DT metal NN has VHZ been VBN unlocked VVN and CC roughed VVD out RP . SENT DINGING VVG HAMMER NN . SENT Specially RB built VVN hammer NN used VVN for IN the DT removal NN of IN the DT smaller JJR dents NNS on IN body NN panels NNS . SENT DIRECT JJ DAMAGE NN . SENT Damage NN that WDT occurs VVZ to TO the DT area NN that WDT is VBZ in IN direct JJ contact NN with IN the DT damaging JJ force NN of IN impact NN . SENT DIRECT JJ PULLING VVG . SENT Pulling VVG on IN the DT damage NN using VVG a DT direct JJ pull NN . SENT DIRT NN NIBS NNS . SENT Small JJ specks NNS of IN foreign JJ material NN in IN a DT dried VVN film NN of IN finishing VVG material NN . SENT They PP should MD be VB removed VVN by IN scuff NN sanding VVG . SENT DIRTY JJ . SENT Opposite JJ of IN clean JJ . SENT Describes VVZ a DT color NN that WDT has VHZ a DT drab JJ appearance NN rather RB than IN one CD with IN a DT bright JJ appearance NN . SENT The DT addition NN of IN black JJ makes NNS colors NNS dirty JJ . SENT DISINTEGRATION NN . SENT Dried VVN film NN of IN a DT finishing JJ material NN completely RB breaks VVZ down RP . SENT DISK NN SANDER NN . SENT Power NN sanding VVG tool NN used VVN for IN grinding VVG , , sanding VVG and CC polishing VVG repaired VVN metal NN areas NNS . SENT It PP is VBZ manufactured VVN in IN either CC the DT 7 CD in RB . SENT standard NN or CC the DT 7 CD and CC 9 CD in RB . SENT heavy JJ duty NN model NN and CC is VBZ available JJ with IN a DT round NN , , flexible JJ , , molded VVN rubber NN , , backing VVG pad NN 5 CD . SENT 7 CD and CC 9 CD inch NN in IN diameter NN . SENT DISK NN TRIMMER JJR . SENT Special JJ tool NN used VVN to TO cut VV down RP a DT worn JJ out IN sanding VVG disk NN to TO a DT somewhat RB smaller JJR size NN , , giving VVG it PP a DT fresh JJ cutting NN edge NN . SENT DOG NN TRACKING NN . SENT Condition NN in IN which WDT a DT vehicle's NNS wheels NNS do VVP not RB follow VV in IN direct JJ line NN but CC at IN an DT angle NN . SENT DOLLY NN . SENT Tool NN that WDT is VBZ made VVN in IN different JJ shapes NNS , , usually RB held VVN in IN one CD hand NN on IN inner JJ side NN of IN a DT dented VVN panel NN while IN the DT outer JJ side NN is VBZ struck VVN with IN another DT dolly NN or CC dinging VVG hammer NN . SENT DOOR NN PANEL NN FLANGE NN . SENT The DT 90 CD degree NN projecting VVG edge NN all RB around IN the DT edge NN of IN a DT door NN replacement NN panel NN , , by IN means NNS of IN which WDT the DT replacement NN panel NN is VBZ attached VVN to TO the DT door NN frame NN or CC inner JJ construction NN . SENT DOUBLE JJ HEAD NN COAT NN . SENT Usually RB called VVN one CD coat NN but CC meaning VVG an DT application NN of IN material NN sprayed VVN horizontally RB and CC immediately RB followed VVN by IN an DT application NN sprayed VVD vertically RB . SENT Also RB called VVN a DT cross NN coat NN . SENT DRIERS NNS . SENT Salts NNS of IN certain JJ metals NNS or CC metallo NN organic JJ compounds NNS , , which WDT when RB added VVD to TO an DT enamel NN , , paint NN , , varnish NN , , or CC oil NN hasten VV the DT drying VVG or CC hardening VVG of IN the DT film NN through IN proper JJ ventilation NN . SENT DRY JJ SPRAY NN . SENT This DT term NN is VBZ used VVN if IN in IN applying VVG a DT finish NN by IN spray NN the DT atomized VVN paint NN is VBZ not RB absorbed VVN in IN the DT film NN , , leaving VVG a DT rough JJ , , dry JJ finish NN . SENT DUCTILITY NN . SENT Refers VVZ to TO the DT property NN whereby WRB a DT material NN can MD be VB worked VVN , , drawn VVN or CC bent NN without IN breaking NN . SENT DURABILITY NN . SENT Life NN of IN a DT paint NN film NN . SENT DUST NN FREE JJ . SENT Condition NN when WRB a DT film NN has VHZ dried VVN so RB that IN it PP will MD no RB longer RB allow VV dust NN to TO penetrate VV and CC stick VV to TO the DT finish NN . SENT E SYM Back RB to TO General NP Terms NNS Index NP ECONOMY NN PART NN . SENT Any DT new JJ vehicle NN part NN of IN accessory JJ that WDT is VBZ purchased VVN from IN a DT source NN other JJ than IN the DT OEM NP parts NNS distribution NN network NN . SENT ECT NNS . SENT Engine NN coolant NN temperature NN sensor NN or CC its PP$ signal NN circuit NN . SENT EGO NN . SENT Exhaust NN gas NN oxygen NN sensor NN or CC its PP$ signal NN circuit NN . SENT EGR NP . SENT Exhaust NN gas NN recirculation NN system NN that WDT is VBZ designed VVN to TO allow VV the DT flow NN of IN inert JJ exhaust NN gases NNS into IN the DT combustion NN chamber NN to TO cool VV the DT combustion NN and CC therefore RB reduce VV the DT amount NN if IN nitrous JJ oxides NNS in IN the DT exhaust NN . SENT ELASTIC JJ LIMIT NN . SENT Amount NN that IN a DT piece NN or CC a DT metal NN panel NN will MD bend VV without IN causing VVG distortion NN or CC separation NN in IN the DT structure NN of IN the DT material NN . SENT ELASTIC JJ METAL NN . SENT All DT V NN channels NNS , , valleys NNS and CC buckles NNS extending VVG outward RB from IN the DT area NN of IN direct JJ damage NN but CC not RB including VVG the DT extreme JJ outer JJ high JJ ridges NNS that IN bound VVN them PP are VBP called VVN elastic JJ metal NN . SENT ELECTRIC JJ HOT JJ KNIFE NN . SENT Type NN of IN electrically RB heated JJ blade NN used VVN to TO cut VV some DT adhesives NNS . SENT ELECTRONIC JJ VEHICLE NN INFORMATION NN CENTER NN . SENT Electronic JJ receiving VVG unit NN that WDT receives VVZ information NN from IN all PDT the DT sensors NNS in IN the DT vehicle NN . SENT EMBLEM NN . SENT Decorative JJ piece NN of IN plastic NN or CC metal NN attached VVN to TO a DT vehicle NN . SENT ENAMEL NN . SENT Pigmented NP alkyd NP varnish NN usually RB characterized VVD by IN a DT glossy JJ surface NN . SENT Dulux NP is VBZ such JJ a DT pigmented JJ synthetic JJ resin NN solution NN . SENT ENERGY NN ABSORBER NN . SENT Device NN used VVN on IN bumpers NNS to TO absorb VV energy NN from IN a DT collision NN . SENT EPOXY JJ RESINS NNS . SENT Resins NNS obtained VVN by IN the DT condensing VVG reaction NN that WDT occurs VVZ between IN phenols NNS and CC epichlorohydrin NN . SENT ESTIMATE NN . SENT The DT written JJ determination NN made VVN by IN an DT appraiser NN or CC estimator NN , , upon IN inspection NN of IN a DT damaged JJ vehicle NN , , regarding VVG the DT cost NN required VVN to TO restore VV the DT vehicle NN to TO the DT condition NN it PP was VBD in RB prior JJ to TO the DT Loss NN . SENT ESTIMATE NN DOCUMENT NN . SENT Form NN on IN which WDT the DT cost NN of IN accomplishing VVG repairs NNS is VBZ written VVN . SENT often RB used VVN as IN the DT basis NN for IN repairs NNS . SENT ESTIMATED JJ TIME NN . SENT Amount NN of IN time NN given VVN to TO repair VV or CC remove VV and CC replace VV an DT item NN or CC part NN . SENT ESTIMATING VVG MANUAL JJ . SENT Manual NP that RB has VHZ the DT information NN on IN the DT replacement NN of IN parts NNS and CC their PP$ standardized JJ lab NN or CC times NNS on IN a DT vehicle NN . SENT ESTIMATOR NN . SENT An DT appraiser NN or CC insurance NN company NN representative NN who WP inspects VVZ a DT damaged JJ vehicle NN and CC determines VVZ the DT cost NN required VVN to TO restore VV the DT vehicle NN to TO the DT condition NN prior RB to TO the DT Loss NN . SENT EVAPORATOR NN . SENT Part NN on IN a DT vehicle NN with IN an DT air NN conditioning NN system NN that WDT causes VVZ the DT refrigerant JJ liquid NN under IN pressure NN to TO change VV to TO gas NN . SENT EXCESS JJ ACETYLENE NN FLAME NN . SENT See VV Carburizing VVG flame NN . SENT EXHAUST NN FAN NN . SENT Fan NN that WDT moves VVZ the DT air NN in IN a DT spray NN booth NN and CC pushes VVZ it PP out RP to TO the DT atmosphere NN . SENT EXHAUST NN SYSTEM NN . SENT System NN of IN many JJ parts NNS used VVN on IN motor NN vehicles NNS to TO move VV the DT gases NNS from IN the DT engine NN to TO the DT rear NN of IN the DT vehicle NN into IN the DT atmosphere NN . SENT EXPANSION NN . SENT Condition NN in IN which WDT an DT object NN becomes VVZ bigger JJR . SENT F SYM Back RB to TO General NP Terms NNS Index NP FACE NN . SENT Appearance NN of IN a DT color NN viewed VVD straight RB on IN . SENT This DT term NN is VBZ most RBS often RB used VVN in IN comparison NN to TO the DT pitch NN of IN a DT color NN , , which WDT is VBZ the DT appearance NN of IN the DT color NN when WRB viewed VVN at IN any DT angle NN other JJ than IN 90 CD degrees NNS . SENT The DT face NN color NN is VBZ often RB different JJ in IN lightness NN or CC darkness NN . SENT FACE NN BAR NN . SENT Large JJ chrome NN plated VVD extrusions NNS that WDT provide VVP protection NN for IN both DT front NN and CC rear NN of IN an DT automobile NN and CC which WDT are VBP generally RB held VVN in IN position NN by IN means NNS of IN brackets NNS bolted VVN to TO the DT side NN rails VVZ of IN the DT frame NN . SENT FADE VV . SENT Denotes VVZ the DT change NN in IN the DT color NN of IN a DT surface NN coating NN where WRB and CC when WRB such PDT a DT coating NN has VHZ been VBN subjected VVN to TO sunlight NN . SENT It PP is VBZ a DT dying VVG away RP or CC bleaching VVG action NN . SENT FALSE JJ STRETCH NN . SENT Bulge NN formed VVD in IN the DT flatter JJR areas NNS of IN an DT outer JJ panel NN whenever WRB the DT collapsed JJ rolled JJ buckle NN in IN the DT crowned VVN surface NN of IN that DT panel NN extends VVZ into IN the DT flatter JJR , , more RBR central JJ portions NNS of IN the DT panel NN in IN the DT area NN of IN indirect JJ damage NN . SENT Even RB after IN the DT damage NN has VHZ been VBN roughed VVN out RP and CC straightened VVD as RB accurately RB as IN possible JJ , , false JJ stretch NN cannot NN be VB completely RB eliminated VVN . SENT FAN NN . SENT Spray NN pattern NN of IN a DT spray NN gun NN . SENT FANNING VVG . SENT Use NN of IN pressurized VVN air NN through IN a DT spray NN gun NN to TO speed VV up RP the DT drying VVG time NN of IN a DT paint NN finish NN . SENT it PP is VBZ not RB recommended VVN . SENT FEATHEREDGE NN SPLITTING NN . SENT Cracks NNS or CC stretch NN marks NNS along IN the DT featheredge NN which WDT occur VVP while IN drying VVG or CC shortly RB after IN the DT topcoat NN has VHZ been VBN applied VVN over IN a DT primer JJR surfacer NN . SENT FEATHEREDGING NP . SENT Sanding VVG down RP a DT surface NN to TO a DT very RB fine JJ edge NN . SENT that DT is VBZ when WRB one CD coat NN of IN material NN is VBZ made VVN gradually RB thinner JJR around IN the DT edge NN until IN it PP finally RB disappears VVZ . SENT FEATHERING NN . SENT Action NN of IN moving VVG a DT spray NN gun NN trigger NN lightly RB at IN each DT end NN of IN a DT stroke NN . SENT FEELING VVG THE DT METAL NN . SENT Used VVN in IN detecting VVG surface NN irregularities NNS . SENT The DT repair NN technician NN slides VVZ the DT palm NN of IN a DT hand NN back RB and CC forth RB over IN the DT work NN and CC is VBZ able JJ to TO detect VV or CC feel VV any DT hollows NNS or CC high JJ spots NNS that WDT may MD be VB present JJ . SENT FENCE NN OFF RB . SENT Method NN of IN shrinking VVG sequence NN to TO prevent VV a DT highly RB stretched VVN metal NN area NN from IN moving VVG . SENT FENDER NN FLANGE NN . SENT Outer JJ rim NN or CC bend VV along RP the DT lower JJR edge NN of IN a DT fender NN that WDT gives VVZ shape NN and CC strength NN to TO the DT side NN of IN the DT fender NN . SENT FERROUS JJ METAL NN . SENT Any DT metal NN composed VVN of IN or CC containing VVG iron NN . SENT FIBERGLASS NNS Very JJ fine JJ staple NN fibers NNS of IN glass NN that WDT are VBP spun VVN together RB . SENT it PP is VBZ used VVN as IN insulation NN and CC for IN repairs NNS on IN automobile NN and CC truck NN bodies NNS . SENT FILING NN . SENT Pushing VVG or CC drawing VVG a DT file NN back RB and CC forth RB over IN the DT surface NN of IN the DT work NN in IN order NN to TO detect VV high JJ and CC low JJ spots NNS surface VVP irregularities NNS or CC to TO wear VV down RP a DT surface NN to TO an DT exact JJ size NN and CC shape NN . SENT FILM NN . SENT A DT layer NN of IN applied VVN coating NN material NN . SENT FILM NN THICKNESS NN . SENT See VV Mil NP FINISH VV COAT NN . SENT The DT last JJ coat NN of IN paint NN to TO be VB applied VVN will MD usually RB determine VV the DT amount NN of IN gloss VV . SENT FISH NN PLATE NN . SENT Repairing VVG of IN a DT cracked VVN frame NN rail NN by IN first JJ of IN all DT welding VVG the DT cracks NNS and CC then RB reinforcing VVG the DT rail NN by IN welding VVG another DT plate NN that WDT covers VVZ and CC extends VVZ well RB beyond IN the DT repaired VVN area NN . SENT FISH NN EYE NN ELIMINATOR NN . SENT Additive JJ put NN in IN paint NN to TO prevent VV the DT occurrence NN of IN fish NN eyes NNS in IN a DT freshly RB painted VVN surface NN . SENT FISHMOUTH NP . SENT Part NN of IN a DT window NN regulator NN where WRB the DT drive NN tape NN is VBZ inserted VVN . SENT FLAKE NN . SENT Particles NNS added VVD to TO a DT color NN to TO achieve VV a DT metallic JJ or CC iridescent JJ finish NN . SENT FLAKING VVG . SENT Condition NN when WRB the DT finish NN does VVZ not RB knit VVN properly RB to TO the DT undercoating VVG , , causing VVG the DT finish NN to TO chip NN off IN the DT work NN by IN breaking VVG into IN small JJ pieces NNS . SENT FLAME NN CUTTING NN . SENT Use NN of IN an DT oxyacetylene NN flame NN to TO cut VV metal NN . SENT FLANGE NN . SENT Projecting VVG edge NN , , rim NN , , or CC bend VV on IN the DT outer JJ edge NN of IN a DT panel NN that WDT stiffens VVZ it PP . SENT FLASH VV BACK RB . SENT Malfunctioning VVG of IN the DT torch NN when WRB the DT flame NN goes VVZ inside IN the DT torch NN and CC it PP starts VVZ to TO hiss VV and CC squeal VV . SENT FLAT JJ . SENT Finish VV that WDT has VHZ no RB luster VV or CC gloss VV . SENT FLAT JJ RATE NN . SENT Piecework NN method NN of IN paying VVG for IN repair NN operations NNS . SENT FLEX NN HEADS NNS . SENT Sometimes RB called VVN rubber NN bases NNS . SENT conform VV to TO any DT contour NN , , and CC are VBP most RBS often RB used VVN as IN a DT terminal JJ point NN for IN pushing VVG against IN concave JJ surfaces NNS . SENT FLINT NN PAPER NN . SENT Inexpensive JJ but CC short JJ working VVG life NN abrasive JJ paper NN , , not RB used VVN extensively RB in IN body NN shops NNS . SENT FLOOD NN . SENT Floating VVG of IN a DT pigment NN to TO the DT surface NN of IN a DT coating NN , , giving VVG a DT changed VVN color NN to TO the DT surface NN and CC lack NN of IN uniformity NN in IN color NN appearance NN through IN the DT film NN . SENT FLOP NN . SENT Appearance NN of IN a DT color NN when WRB viewed VVN from IN any DT angle NN other JJ than IN straight RB on IN . SENT The DT flop NN of IN a DT color NN is VBZ also RB referred VVN to TO as IN its PP$ pitch NN . SENT The DT pitch NN is VBZ often RB different JJ from IN the DT face NN when WRB working VVG with IN iridescent JJ colors NNS . SENT FLOW NN . SENT Ability NN of IN paint NN droplets NNS to TO melt VV or CC merge VV together RB to TO form VV a DT smooth JJ paint NN film NN . SENT FLUID JJ CONTAINERS NNS . SENT Containers NNS designed VVN to TO store VV different JJ types NNS of IN fluids NNS . SENT FLUID JJ NEEDLE NN . SENT Part NN in IN a DT spray NN gun NN that WDT opens VVZ and CC closes VVZ fluid JJ passages NNS . SENT FLUID JJ NEEDLE NN ADJUSTMENT NN . SENT Adjusting VVG the DT amount NN of IN fluid NN that WDT will MD go VV through IN the DT opening NN of IN the DT fluid JJ tip NN . SENT FLUID JJ TIP NN . SENT Part NN of IN a DT spray NN gun NN that IN meters NNS and CC directs VVZ the DT fluid JJ stream NN . SENT FOG NN COAT NN . SENT Thin JJ , , highly RB atomized VVN coat NN applied VVN in IN such PDT a DT way NN as RB to TO obtain VV a DT fast JJ flash NN off RP . SENT and CC thereby RB achieve VV a DT minimum JJ penetration NN of IN the DT thinner JJR into IN the DT old JJ finish NN . SENT FORCE NN DRY JJ . SENT See VV Baking VVG FORGING VVG . SENT Repair NN operation NN used VVN in IN restoring VVG welded VVN butt NN joints NNS to TO as RB near JJ as IN possible JJ the DT same JJ thickness NN and CC molecular JJ structure NN as IN that WDT possessed VVD by IN the DT surrounding VVG sheet NN metal NN . SENT FRAME NN ALIGNMENT NN . SENT Procedure NN by IN which WDT the DT frame NN of IN a DT car NN , , truck NN or CC bus NN that WDT has VHZ been VBN damaged VVN in IN an DT accident NN , , or CC from IN wear NN , , is VBZ restored VVN to TO the DT manufacturer's JJ specifications NNS . SENT FRAME NN GAUGES VVZ . SENT Used VVN in IN determining VVG the DT type NN of IN misalignment NN that WDT has VHZ occurred VVN and CC also RB the DT extent NN of IN the DT damage NN . SENT FRAME NN HORNS NNS . SENT Extending VVG ends NNS of IN the DT side NN rails VVZ of IN a DT frame NN to TO which WDT the DT bumper NN brackets NNS are VBP fastened VVN . SENT FRAME NN RACK NN . SENT Equipment NN used VVD to TO repair VV damaged JJ frame NN and CC unibody NN members NNS . SENT FRONT JJ END NN SHEET NN METAL NN . SENT All DT parts NNS from IN the DT cowl NN assembly NN forward RB are VBP considered VVN front JJ end NN sheet NN metal NN . SENT This DT includes VVZ the DT grille NN , , the DT hood NN , , and CC right RB and CC left VVN fender NN and CC the DT front JJ bumper NN assembly NN . SENT FUSIBLE JJ LINK NN . SENT Wire NN designed VVN to TO open VV a DT circuit NN by IN melting NN , , when WRB too RB much JJ current JJ flows NNS through IN it PP . SENT FUSION NN WELD NN . SENT Operation NN in IN which WDT two CD pieces NNS of IN the DT same JJ kind NN of IN metal NN are VBP made VVN into IN one CD is VBZ called VVN fusion NN welding VVG . SENT G NP Back RB to TO General NP Terms NNS Index NP GARNET NN PAPER NN . SENT Hard RB , , sharp JJ , , red JJ abrasive NN . SENT more RBR expensive JJ than IN flint NN paper NN but CC will MD last VV much RB longer RBR . SENT GARNISH NN MOLDINGS NNS . SENT Moldings NNS that WDT fit VVP around IN the DT inside NN of IN door NN , , windshield NN and CC rear JJ window NN openings NNS , , generally RB held VVN in IN position NN by IN countersunk VVN metal NN screws NNS . SENT GEL NN . SENT General JJ consistency NN of IN a DT jelly NN . SENT the DT material NN being VBG soft JJ but CC not RB free JJ flowing VVG . SENT The DT term NN gel NN is VBZ generally RB applied VVN to TO a DT vehicle NN as RB contrasted VVN to TO false JJ body NN caused VVN by IN pigmentation NN . SENT GLASS NN RUN NN CHANNEL NN . SENT Part NN used VVD in IN the DT doors NNS where WRB glass NN moves VVZ up RP and CC down RB that WDT prevents VVZ the DT glass NN from IN being VBG damaged VVN . SENT GLAZING NN . SENT Application NN of IN a DT filler NN by IN means NNS of IN a DT putty JJ knife NN , , the DT material NN being VBG filled VVN into IN the DT depression NN but CC scraped VVD off RP the DT higher JJR areas NNS . SENT GLOSS VV . SENT Shine NN , , sheen NN , , or CC luster VV of IN a DT dry JJ film NN . SENT GRILLE NN . SENT Open JJ work NN structure NN made VVD out RP of IN plastic NN , , die VV cast NN , , aluminum NN or CC stamped VVD out RP of IN sheet NN which WDT covers VVZ the DT air NN intake NN opening NN in IN front NN of IN the DT radiator NN , , but CC allows VVZ the DT air NN to TO pass VV freely RB through IN it PP . SENT GRITTY JJ . SENT A DT product NN is VBZ said VVN to TO be VB gritty JJ when WRB it PP contains VVZ large JJ particles NNS , , either CC from IN insufficient JJ grinding VVG , , which WDT would MD mean VV seed NN , , or CC by IN the DT presence NN of IN large JJ , , hard JJ particles NNS of IN foreign JJ materials NNS . SENT GROMMET NN . SENT Rubber NN or CC plastic NN insulator NN used VVN to TO protect VV electrical JJ wires NNS or CC other JJ lines NNS from IN being VBG damaged VVN by IN the DT sheet NN metal NN edge NN . SENT GROUND NN CABLE NN . SENT The DT ground NN cable NN clamped VVN to TO the DT work NN allows VVZ the DT electric JJ current NN produced VVN by IN the DT welding VVG machine NN to TO flow VV through IN the DT electrode NN cable NN and CC the DT electrode NN to TO the DT work NN when WRB the DT arc NN is VBZ formed VVN . SENT The DT current NN completes VVZ its PP$ circuit NN by IN flowing VVG through IN the DT ground NN cable NN back RB to TO the DT welding VVG machine NN . SENT GROUND NN ELECTRICITY NN . SENT Part NN of IN the DT circuit NN that WDT allows VVZ the DT current JJ to TO return VV to TO the DT negative JJ terminal NN of IN the DT battery NN . SENT GUIDE NN COAT NN . SENT Coat NN of IN a DT different JJ color NN from IN the DT other JJ coat NN is VBZ used VVN to TO serve VV as IN a DT guide NN coat NN in IN rubbing VVG or CC sanding VVG to TO determine VV when WRB a DT smooth JJ surface NN has VHZ been VBN reached VVN . SENT GUMMING VVG . SENT Condition NN where WRB the DT sandpaper NN becomes VVZ clogged VVN by IN the DT abraded VVN surface NN coating NN . SENT Compare VV Caking VVG . SENT GUN NN BODY NN . SENT Part NN of IN the DT spray NN gun NN to TO which WDT all DT required JJ parts NNS are VBP bolted VVN or CC attached VVN . SENT H NP Back RB to TO General NP Terms NNS Index NP HAIRLINING NP . SENT Very RB fine JJ lines NNS or CC checks NNS on IN the DT dried VVN surface NN coating NN of IN a DT finished JJ material NN . SENT HARDENER NN . SENT Special JJ additive NN designed VVN to TO promote VV a DT faster JJR cure NN of IN the DT enamel NN paint NN film NN . SENT HARDNESS NN . SENT Quality NN of IN the DT paint NN film NN that WDT gives VVZ it PP resistance NN to TO surface VV damage NN . SENT HATCHBACK NN . SENT Part NN used VVD on IN a DT vehicle NN to TO close VV the DT rear JJ section NN . SENT HEADER NN BAR NN . SENT Framework NN or CC inner JJ construction NN that WDT joins VVZ the DT upper JJ sections NNS of IN the DT windshield NN , , pillars NNS , , forms VVZ the DT upper JJ portion NN of IN the DT windshield NN opening NN and CC reinforces VVZ the DT turret NN top JJ panel NN . SENT HEADLIGHT NN . SENT Light NN used VVD to TO light VV the DT road NN ahead RB of IN a DT vehicle NN . SENT HEADLINING VVG . SENT Different JJ types NNS of IN materials NNS used VVN to TO cover VV the DT inner JJ surface NN of IN the DT roof NN in IN a DT car NN . SENT HIDE VV GLUE NN . SENT Made VVN from IN animal JJ hides NNS and CC used VVN in IN making VVG abrasives NNS that WDT can MD only RB be VB used VVN in IN dry JJ sanding VVG and CC grinding VVG work NN . SENT HIDING NN . SENT The DT hiding NN power NN of IN a DT finishing JJ material NN is VBZ a DT measure NN of IN its PP$ opacity NN or CC its PP$ ability NN to TO cover VV solidly RB over IN another DT color NN as RB to TO obscure VV or CC prevent VV the DT original JJ color NN from IN showing VVG through RP . SENT HIGH JJ CROWN NN METAL NN . SENT Outward RB curving VVG portion NN of IN a DT body NN panel NN . SENT HINGE VV EFFECT NN . SENT Effect NN of IN expansion NN and CC contraction NN that WDT causes VVZ the DT metal NN to TO move VV as RB if IN it PP was VBD on IN a DT hinge NN . SENT HINGE VV PILLAR NN . SENT Framework NN or CC inner JJ construction NN to TO which WDT the DT door NN hinges VVZ fasten VV . SENT HOLD VV OUT RP . SENT Ability NN of IN a DT surface NN to TO keep VV the DT topcoat NN from IN sinking VVG in RP . SENT HOOD NN PANEL NN . SENT Large JJ metal NN panel NN that WDT generally RB fills VVZ in IN the DT space NN between IN the DT two CD fenders NNS and CC covers VVZ over IN the DT engine NN compartment NN . SENT HSLA NP HIGH JJ STRENGTH NN LOW JJ ALLOY NN . SENT Type NN of IN steel NN with IN low JJ alloy NN used VVN in IN the DT fabricating VVG of IN certain JJ parts NNS for IN motor NN vehicles NNS . SENT HSS NP HIGH JJ STRENGTH NN STEEL NN . SENT Type NN of IN steel NN used VVN that DT is VBZ very RB strong JJ , , but CC is VBZ thin JJ and CC light JJ . SENT HUE NN . SENT Basic JJ color NN that WDT is VBZ blue JJ , , red JJ , , yellow JJ , , green JJ , , violet NN , , or CC orange NN . SENT Hue NP is VBZ used VVN to TO determine VV where WRB the DT color NN would MD fall VV generally RB on IN the DT color NN wheel NN . SENT HUMIDITY NN . SENT Water NN vapor NN present JJ in IN the DT air NN in IN varying VVG amounts NNS . SENT HVLP NP HIGH JJ VOLUME NN , , LOW JJ PRESSURE NN . SENT Type NN of IN spraying VVG system NN that WDT uses VVZ a DT high JJ volume NN and CC low JJ pressure NN of IN atomizing VVG air NN to TO apply VV material NN to TO a DT surface NN . SENT Reduces VVZ over IN spray NN of IN product NN into IN the DT atmosphere NN . SENT HYDRAULIC JJ JACKING VVG UNIT NN . SENT System NN of IN using VVG a DT hydraulic JJ pump NN , , hose NN , , ram NN , , and CC required VVN attachments NNS to TO provide VV the DT transfer NN of IN hydraulic JJ power NN . SENT HYDRAULIC JJ OIL NN . SENT Special JJ type NN of IN oil NN used VVN in IN hydraulic JJ systems NNS that WDT does VVZ not RB deteriorate VV or CC attack VV the DT rubber NN seals NNS in IN the DT jack NN or CC its PP$ hose NN . SENT I PP Back RB to TO General NP Terms NNS Index NP INDIRECT JJ DAMAGE NN . SENT Any DT damage NN that WDT occurs VVZ as IN a DT result NN of IN direct JJ damage NN . SENT INDUCTION NN BAKING VVG . SENT Heat NN used VVN for IN baking VVG finishes NNS , , induced VVN by IN electrostatic JJ or CC electromagnetic JJ means NNS . SENT INDUSTRIAL JJ FALLOUT NN . SENT Chemical NN compounds NNS present JJ in IN the DT air NN which WDT are VBP deposited VVN on IN the DT horizontal NN surfaces VVZ of IN vehicles NNS and CC which WDT under IN certain JJ circumstances NNS will MD affect VV the DT finish NN , , particularly RB metallics NNS . SENT INNER JJ CONSTRUCTION NN . SENT Framework NN and CC inner JJ panels NNS that WDT hold VVP and CC reinforce VVP the DT outer JJ body NN panels NNS . SENT INNER JJ SKIRT NN . SENT Part NN used VVD in IN the DT front JJ section NN of IN a DT vehicle NN between IN the DT upper JJ and CC lower JJR rails NNS . SENT INSERT NN . SENT Fabricated VVN part NN used VVN to TO reinforce VV a DT section NN when WRB it PP is VBZ being VBG sectioned VVN . SENT INTAKE NN FILTERS NNS . SENT Filters NNS used VVD where WRB the DT air NN enters VVZ the DT spray NN booth NN to TO remove VV the DT dust NN in IN the DT air NN stream NN . SENT IRIDESCENTS NNS . SENT All DT colors NNS that WDT contain VVP aluminum NN , , mica NN , , or CC other JJ particles NNS that WDT impart VV a DT metallic JJ appearance NN to TO the DT color NN . SENT Used VVN interchangeably RB with IN the DT word NN metallic JJ . SENT Iridescent JJ colors NNS must MD be VB carefully RB matched VVN on IN the DT face NN and CC the DT pitch NN in IN order NN to TO achieve VV a DT desirable JJ appearance NN . SENT ISOCYANATE NN . SENT Additive NN that WDT is VBZ part NN of IN many JJ paint NN and CC plastic NN hardeners NNS . SENT injurious JJ to TO the DT lungs NNS . SENT J NP Back RB to TO General NP Terms NNS Index NN JERKY JJ OR CC FLUTTERING VVG SPRAY NN . SENT Intermittent JJ amount NN of IN fluid NN delivered VVN by IN a DT spray NN gun NN . SENT occurs VVZ in IN the DT suction NN feed NN type NN . SENT JIG NN . SENT Mechanical JJ device NN for IN holding VVG work NN in IN its PP$ exact JJ position NN while IN it PP is VBZ being VBG welded VVN . SENT JIGSAW NN . SENT Narrow JJ bladed NN saw VVD usually RB driven VVN by IN an DT electric JJ motor NN . SENT Used VVN to TO cut VV body NN panels NNS . SENT K NP KNIT VVN . SENT Adhere VV or CC bond NN together RB . SENT L NP LACQUER NN . SENT Refinishing VVG material NN that WDT dries VVZ by IN the DT evaporation NN of IN the DT thinner JJR . SENT LAP NN . SENT Point VV where WRB one CD coat NN extends VVZ over IN another DT . SENT LAP NN WELD NN . SENT Type NN of IN weld NN made VVN by IN overlapping JJ two CD pieces NNS of IN metal NN and CC joining VVG them PP by IN running VVG a DT bead NN along IN only RB one CD of IN the DT edges NNS . SENT LATERAL JJ RUNOUT NP . SENT Amount NN a DT wheel NN moves VVZ from IN side NN to TO side VV when WRB rotated VVD , , due JJ to TO being VBG bent JJ . SENT LEAD JJ TIRE NN . SENT A DT pulling VVG condition NN in IN a DT radial JJ tire NN causing VVG the DT steering NN to TO want VV to TO turn VV to TO that DT side NN when WRB rotated VVD . SENT LET VV DOWN RP PANEL NN . SENT Panel NN made VVD by IN a DT paint NN technician NN with IN different JJ methods NNS of IN application NN and CC amounts NNS of IN material NN , , resulting VVG in IN different JJ shades NNS of IN the DT same JJ color NN . SENT LEVELING VVG OUT RP . SENT Flowing VVG or CC settling VVG to TO a DT smooth JJ , , uniform JJ surface NN . SENT LIFTING NN . SENT Disruption NN of IN a DT paint NN film NN by IN the DT application NN of IN a DT succeeding VVG coat NN , , caused VVN by IN the DT solvents NNS of IN the DT succeeding VVG coat NN penetrating VVG and CC partially RB dissolving VVG or CC swelling VVG the DT preceding VVG dried VVN film NN . SENT LIGHTEN VV . SENT Addition NN of IN white JJ to TO make VV solid JJ colors NNS lighter JJR . SENT the DT addition NN of IN metallic JJ flakes NNS makes VVZ metallic JJ colors NNS lighter JJR . SENT LISTING NN BOWS NNS . SENT Slightly RB tempered VVN , , bowed VVD steel NN rods NNS that WDT are VBP inserted VVN into IN headlinings NNS to TO keep VV them PP in IN proper JJ position NN inside IN the DT passenger NN compartment NN . SENT LIVERING NP . SENT Coagulation NN of IN paint NN into IN a DT viscous JJ liver NN like IN mass NN . SENT LOAD NN VOLTAGE NN TEST NN . SENT Test NN given VVN to TO a DT battery NN to TO find VV its PP$ condition NN . SENT LOCKSTRIP NN . SENT Part NN of IN a DT weatherstrip NN that WDT applies VVZ pressure NN to TO keep VV the DT windshield NN or CC glass NN in IN position NN . SENT LOW JJ CROWN NN METAL NN . SENT Portion NN of IN a DT body NN panel NN with IN just RB a DT very RB small JJ amount NN of IN outward RB curve NN . SENT LOWER RBR INNER JJ AND CC OUTER JJ RAILS NNS . SENT Parts NNS used VVN in IN the DT front JJ structure NN of IN the DT vehicle NN to TO give VV the DT assembly NN the DT required VVN strength NN to TO hold VV the DT other JJ parts NNS . SENT LUSTER VV . SENT Gloss VV of IN sheen NN of IN a DT finish NN . SENT M NP Back RB to TO General NP Terms NNS Index NP MACPHERSON NP STRUT NN . SENT Type NN of IN suspension NN using VVG a DT lower JJR control NN arm NN and CC an DT upright JJ shock NN absorber NN assembly NN , , spring NN , , and CC spindle NN . SENT MAKEUP NN AIR NN . SENT System NN that WDT brings VVZ and CC heats VVZ air NN from IN outside NN to TO a DT desired VVN air NN flow NN and CC temperature NN . SENT MAP NN . SENT Manifold JJ Absolute JJ Pressure NN sensor NN or CC its PP$ signal NN circuit NN . SENT MASH NN . SENT Type NN of IN frame NN damage NN in IN which WDT a DT portion NN of IN the DT side NN rail NN is VBZ bent JJ down IN causing VVG buckles NNS to TO be VB formed VVN on IN the DT underside NN . SENT MASKING VVG . SENT Application NN of IN paper NN or CC other JJ material NN and CC masking VVG tape NN to TO cover VV an DT object NN that WDT must MD be VB protected VVN from IN overspray NN . SENT MASKING VVG PAPER NN . SENT Paper NN designed VVN to TO prevent VV paint NN bleeding VVG through RP and CC resist VV water NN soaking VVG to TO a DT certain JJ degree NN . SENT MASKING VVG TAPE NN . SENT Special JJ paper NN that WDT is VBZ coated VVN with IN adhesive NN used VVN to TO protect VV body NN parts NNS or CC to TO attach VV masking VVG paper NN to TO the DT car NN . SENT MASTER NN CYLINDER NN . SENT Part NN of IN the DT brake NN system NN that WDT stores VVZ the DT brake NN fluid NN and CC when WRB the DT pedal NN is VBZ depressed VVN , , forces VVZ the DT fluid NN to TO the DT cylinders NNS in IN the DT wheel NN assembly NN . SENT MATCHING VVG . SENT In IN painting NN , , to TO make VV colors NNS look VV the DT same JJ . SENT METAL NN CONDITIONER NN . SENT Acetic JJ acid NN preparation NN that WDT is VBZ used VVN to TO prepare VV metal NN , , remove VV rust NN , , and CC etch VV the DT metal NN slightly RB to TO provide VV a DT good JJ adherence NN between IN the DT metal NN and CC the DT paint NN . SENT METAL NN FINISHING VVG . SENT Operation NN in IN which WDT hidden JJ surface NN irregularities NNS are VBP detected VVN and CC removed VVN by IN means NNS of IN filing VVG and CC picking VVG the DT straightened VVN metal NN unit NN all DT low JJ spots NNS have VHP been VBN eliminated VVN and CC a DT perfectly RB smooth JJ and CC level NN surface NN is VBZ obtained VVN . SENT METAL NN STAMPING VVG . SENT Process NN of IN manufacturing VVG auto NN body NN parts NNS in IN which WDT straight JJ sheets NNS of IN metal NN are VBP placed VVN in RP between IN dies VVZ operated VVN by IN huge JJ presses NNS and CC die VV formed VVN or CC stamped VVN into IN the DT finished JJ part NN . SENT METALLIC JJ . SENT General JJ term NN applied VVN to TO finishes NNS containing VVG aluminum NN particles NNS . SENT MIG NN METAL NN INERT JJ GAS NN WELDING VVG . SENT Continuous JJ welding VVG system NN that WDT uses VVZ the DT electrical JJ arc NN and CC gas NN to TO protect VV the DT weld NN . SENT MIL NN . SENT Measure NN of IN film NN thickness NN equal JJ to TO 0 CD . SENT 001 CD inches NNS . SENT MILKINESS NN . SENT Cloudy JJ , , whitish JJ , , not RB clear JJ . SENT MIST NN COAT NN . SENT Light JJ spray NN coat NN of IN volatile JJ solvent JJ by IN itself PP or CC with IN very RB little JJ color NN in IN it PP . SENT MODIFIED VVN UNITIZED JJ BODY NN CONSTRUCTION NN . SENT Form NN of IN body NN construction NN consisting VVG of IN half DT frame NN and CC half DT unitized JJ body NN construction NN . SENT MOLDINGS NNS . SENT Metal NN or CC plastic NN parts NNS used VVN to TO beautify VV a DT vehicle NN or CC to TO protect VV the DT panels NNS from IN damage NN . SENT MOTTLING VVG . SENT Striped JJ or CC spotty JJ appearance NN that WDT occurs VVZ in IN metallics NNS when WRB the DT flakes NNS flow VVP together RB because IN of IN poor JJ spraying VVG techniques NNS . SENT MURIATIC JJ ACID NN . SENT Sometimes RB called VVN hydrochloric JJ acid NN . SENT A DT strong JJ acid NN used VVN for IN cleaning VVG metal NN and CC when WRB cut NN is VBZ used VVN for IN soldering VVG . SENT N NP Back RB to TO General NP Terms NNS Index NP NAMEPLATES NNS . SENT Ornaments NNS with IN the DT vehicle's NNS name NN that WDT is VBZ used VVN to TO identify VV the DT make VVP of IN the DT vehicle NN . SENT NATURAL JJ MINERAL NN ABRASIVE NN . SENT Abrasive NN made VVD from IN materials NNS found VVN in IN nature NN . SENT NEUTRAL JJ FLAME NN . SENT Oxyacetylene NN flame NN burning VVG equal JJ parts NNS of IN acetylene NN and CC oxygen NN . SENT NITROCELLULOSE NN . SENT Gun NN cotton NN or CC proxylin NN . SENT a DT compound NN of IN nitrogen NN and CC cellulose NN prepared VVN from IN nitric JJ acid NN and CC cotton NN or CC wood NN fiber NN . SENT NONELASTIC JJ METAL NN AREAS NNS . SENT Areas NNS in IN auto NN body NN panels NNS that WDT have VHP been VBN permanently RB deformed VVN and CC that DT will MD not RB spring VV back RB to TO their PP$ original JJ shape NN after IN stresses NNS and CC strains NNS have VHP been VBN released VVN . SENT NONFERROUS JJ METALS NNS . SENT Metals NNS that WDT contain VVP no DT iron NN . SENT NORMALIZING VVG . SENT Removing VVG of IN stresses NNS and CC strains NNS in IN metal NN . SENT This DT is VBZ done VVN by IN hammering NN , , heating VVG up RP the DT metal NN , , or CC by IN a DT combination NN of IN both DT . SENT O NP O NP . SENT E SYM . SENT M NP . SENT . SENT Original JJ equipment NN manufacturer NN . SENT Usually RB refers VVZ to TO replacement NN parts NNS for IN a DT vehicle NN that WDT were VBD made VVN by IN the DT same JJ manufacturer NN as IN the DT car NN , , rather RB than IN replacement NN parts NNS made VVN by IN a DT different JJ manufacturer NN . SENT OFFSET VVN . SENT Part NN that WDT has VHZ an DT abrupt JJ change NN in IN dimension NN or CC profile NN of IN an DT object NN . SENT OHMMETER NN . SENT Electronic JJ gauge NN used VVN to TO measure VV resistance NN of IN an DT electrical JJ circuit NN or CC part NN . SENT OPAQUE JJ . SENT Impervious JJ to TO light NN . SENT not RB transparent JJ . SENT OPEN JJ CIRCUIT NN . SENT Break NN or CC open JJ condition NN in IN an DT electric JJ circuit NN that WDT interrupts VVZ current JJ flow NN . SENT OPEN JJ COAT NN . SENT Noncontiguous JJ spacing NN of IN the DT grit NN on IN sandpaper NN or CC grinding VVG disk NN . SENT OPEN JJ TIME NN . SENT Term NN used VVN in IN repairs NNS when WRB the DT time NN cannot NN be VB estimated VVN and CC the DT employee NN uses VVZ a DT clock NN to TO calculate VV the DT amount NN of IN time NN required VVN to TO accomplish VV the DT repair NN . SENT ORANGE JJ PEEL NN . SENT Uneven JJ , , pebbly JJ surface NN somewhat RB resembling VVG the DT skin NN of IN an DT orange NN . SENT appears VVZ in IN a DT paint NN film NN that WDT has VHZ been VBN applied VVN by IN spray NN . SENT ORBITAL JJ SANDER NN . SENT Type NN of IN sander NN that WDT uses VVZ an DT orbit NN motion NN to TO accomplish VV the DT sanding VVG of IN different JJ materials NNS . SENT ORIGINAL JJ FINISH NN . SENT Paint VV the DT car NN manufacturer NN applies VVZ at IN the DT factory NN . SENT OVERALL RB REPAINTING VVG . SENT Refinish JJ repair NN job NN in IN which WDT the DT whole JJ vehicle NN is VBZ completely RB repainted VVN . SENT OVERLAP VV . SENT Amount NN of IN the DT spray NN pattern NN that WDT covers VVZ the DT previous JJ spray NN swath NN . SENT OVERSPRAY NP . SENT See VV Dry NP Spray NP . SENT OXIDATION NN . SENT The DT act NN or CC process NN of IN combining VVG with IN oxygen NN . SENT OXIDIZING VVG FLAME NN . SENT Oxyacetylene NN flame NN that WDT uses VVZ more JJR oxygen NN than IN acetylene NN in IN its PP$ flame NN . SENT OXYACETYLENE NN WELDING VVG . SENT Process VV where WRB oxygen NN and CC acetylene NN are VBP burned VVN using VVG a DT torch NN to TO produce VV a DT flame NN hot JJ enough RB to TO melt VV metal NN . SENT P NN Back RB to TO General NP Terms NNS Index NP PAINT NN ARRESTOR NN . SENT Filter NP used VVD to TO clean VV the DT air NN of IN paint NN fumes NNS before IN it PP is VBZ exhausted VVN . SENT PAINT NN FILM NN . SENT Coating NN of IN paint NN that WDT is VBZ applied VVN to TO a DT material NN . SENT PAINT NN REMOVER NN . SENT Fast RB acting VVG blend NN of IN solvent JJ used VVN to TO remove VV enamels NNS , , lacquers NNS and CC varnish NN . SENT PAINT NN STRAINER NN . SENT Filter NP used VVD to TO clean VV paint NN as IN it PP is VBZ poured VVN into IN the DT gun NN cup NN . SENT PARALLEL JJ CIRUIT NN . SENT Circuit NN that WDT provides VVZ more JJR than IN one CD path NN for IN the DT current JJ to TO flow VV . SENT PARTIAL JJ REPAIR NN PROCEDURE NN . SENT Procedure NN used VVD in IN painting NN when WRB only RB a DT part NN of IN the DT panel NN is VBZ painted VVN . SENT PCV NP . SENT System NN that WDT controls VVZ the DT flow NN of IN crankcase NN vapors NNS into IN the DT engine NN intake NN manifold NN , , where WRB they PP are VBP burned VVN in IN combustion NN rather RB than IN being VBG discharged VVN into IN the DT atmosphere NN . SENT PEARL VV LUSTER VV . SENT Paint NN system NN that WDT uses VVZ mica NN chips NNS to TO give VV a DT pearl JJ effect NN in IN the DT paint NN film NN . SENT PEBBLING NN . SENT Excessively RB large JJ orange NN peel NN . SENT PEELING NN . SENT Loss NN of IN bond NN or CC adhesion NN of IN paint NN film NN from IN the DT surface NN to TO which WDT it PP is VBZ applied VVN . SENT PENETRATION NN . SENT Term NN often RB used VVN in IN welding VVG to TO indicate VV how WRB deep JJ the DT weld NN has VHZ penetrated VVN the DT metal NN . SENT PERCHLORETHYLENE NP . SENT Solvent JJ used VVN in IN determining VVG whether IN the DT finish NN is VBZ acyrlic JJ lacquer NN , , nitrocellulose NN lacquer NN , , or CC enamel NN . SENT PHENOLIC JJ RESIN NN . SENT Resin NN that WDT is VBZ based VVN on IN the DT reaction NN between IN formaldehyde NN and CC phenol NN . SENT PICKING VVG . SENT Raising VVG up RP low JJ spots NNS with IN the DT sharp JJ pointed JJ end NN of IN a DT pick NN hammer NN . SENT PICKS NNS . SENT Special JJ tools NNS used VVN in IN the DT metal NN finishing VVG operation NN for IN raising VVG low JJ spots NNS located VVN in IN the DT more JJR central JJ areas NNS of IN inaccessible JJ body NN panels NNS . SENT PIERCING VVG . SENT Small JJ holes NNS in IN door NN panels NNS into IN which WDT special JJ nylon NN clips NNS used VVN to TO hold VV the DT weatherstrip NN are VBP forced VVN or CC pushed VVN in IN . SENT PIGMENT NN . SENT Any DT fine NN , , insoluble JJ , , dry JJ , , solid JJ particles NNS used VVN to TO impart VV color NN . SENT PILING VVG . SENT Heaping VVG , , or CC applying VVG too RB heavily RB . SENT PIN VV SHRINK VV . SENT Very RB small JJ type NN of IN shrink VV used VVN for IN delicate JJ shrinking VVG purposes NNS . SENT PINCH NN WELD NN FLANGE NN . SENT Flange NN that WDT is VBZ formed VVN when WRB the DT framework NN and CC outer JJ panels NNS are VBP clamped VVN and CC spot NN welded VVN together RB as RB found VVN on IN windshield NN and CC rear JJ window NN openings NNS . SENT PINCH NN WELD NN PRIMER NN . SENT Primer NP used VVD on IN a DT pinch NN weld NN before IN applying VVG the DT adhesive NN for IN better JJR adhesion NN . SENT PINHOLING VVG AND CC PITTING VVG . SENT Minute NN hollows NNS or CC holes NNS no RB larger JJR than IN the DT head NN of IN a DT pin NN in IN a DT film NN produced VVN by IN the DT bursting VVG of IN trapped JJ air NN , , moisture NN , , or CC thinner JJR during IN drying VVG . SENT PITCH NN . SENT Appearance NN of IN a DT color NN when WRB viewed VVN from IN any DT angle NN other JJ than IN straight RB on IN . SENT Most RBS often RB used VVN in IN comparison NN to TO the DT face NN of IN a DT color NN , , which WDT is VBZ the DT appearance NN of IN the DT color NN when WRB viewed VVN at IN a DT 90 CD degree NN angle NN or CC straight RB on IN . SENT Pitch NN is VBZ also RB referred VVN to TO as IN the DT flop NN of IN a DT color NN . SENT The DT pitch NN is VBZ often RB different JJ from IN the DT face NN when WRB working VVG with IN iridescent JJ colors NNS . SENT PLASMA NN TORCH NN . SENT Arc JJ torch NN used VVN to TO cut VV metal NN . SENT PLASTIC JJ FILLER NN . SENT Compound NN of IN resin NN and CC fiberglass NNS used VVN to TO fill VV dents NNS on IN car NN bodies NNS . SENT PLUNGER NN . SENT Male NN threaded VVD part NN , , that WDT acts VVZ like IN a DT piston NN moving VVG in RP and CC out RP of IN the DT ram NN body NN and CC onto IN which WDT different JJ lengths NNS of IN extension NN tubing NN and CC attachments NNS can MD be VB connected VVN . SENT POLYCHROMATIC JJ . SENT Term NN used VVD by IN some DT paint NN manufacturers NNS for IN color NN coats NNS that WDT contain VVP aluminum JJ powder NN in IN flake NN form NN . SENT POLYESTER NN FILLER NN . SENT Special JJ kind NN of IN putty NN like IN filler NN used VVN in IN filling VVG slight JJ imperfections NNS and CC low JJ spots NNS on IN panels NNS . SENT POLYESTER NN RESIN NN . SENT Bonding VVG liquid NN that WDT forms VVZ a DT good JJ bond NN with IN fiberglass NNS surfaces VVZ only RB . SENT POLYMERIZATION NN . SENT Drying VVG of IN enamel NN by IN formation NN of IN a DT polymer NN from IN monomers NNS . SENT POLYOLEFIN NP . SENT A DT plastic JJ material NN used VVN to TO make VV flexible JJ bumper NN covers VVZ . SENT POLYURETHANE NN . SENT Chemical NN structure NN used VVN in IN the DT production NN of IN resins NNS for IN enamel NN paint NN finishes NNS . SENT also RB used VVN for IN some DT plastic JJ bumper NN covers VVZ . SENT POOR JJ ADHESION NN . SENT Material NN that WDT has VHZ poor JJ bond NN to TO the DT underlying JJ surface NN . SENT POP NN RIVET NN . SENT Rivet NN that WDT uses VVZ a DT mandrel NN that WDT is VBZ pulled VVN out RP by IN a DT special JJ tool NN to TO collapse VV and CC set VV a DT rivet NN . SENT POWDERED JJ FIBERGLASS NNS . SENT Processed JJ fiberglass NNS that WDT has VHZ been VBN crushed VVN into IN a DT powder NN . SENT It PP not RB only RB gives VVZ bulk NN but CC also RB strength NN to TO the DT filler NN . SENT POWER NN STEERING NN PUMP NN . SENT Pump NN driven VVN by IN the DT engine NN which WDT uses VVZ fluid JJ to TO help VV turn VV the DT front JJ wheels NNS . SENT POWER NN TRAIN NN . SENT Motor NP , , transmission NN , , and CC drive NN assembly NN , , especially RB on IN front JJ wheel NN drive NN vehicles NNS . SENT PRESSURE NN FEED NN GUN NN . SENT Spray NN gun NN equipped VVN with IN a DT separate JJ paint NN container NN that WDT is VBZ pressurized VVN and CC connected VVN to TO the DT spray NN gun NN by IN means NNS of IN two CD hoses NNS . SENT PRIMARY JJ COLORS NNS . SENT Main JJ colors NNS from IN which WDT other JJ colors NNS are VBP formulated VVN . SENT PRIMER JJR . SENT Undercoat NN applied VVD to TO improve VV the DT adhesion NN of IN the DT color NN coat NN . SENT PRIMER JJR COAT NN . SENT Used VVN in IN a DT paint NN system NN to TO improve VV adhesion NN . SENT requires VVZ sanding VVG . SENT PRIMER JJR SEALER NN . SENT Undercoat NN that WDT improves VVZ the DT adhesion NN of IN the DT topcoat NN and CC seals NNS the DT old JJ painted JJ surfaces VVZ . SENT PRIMER JJR SURFACER NN . SENT High JJ solid JJ type NN of IN primer NN used VVN to TO fill VV small JJ imperfections NNS in IN a DT substrate NN . SENT PUBLIC JJ LIABILITY NN . SENT Type NN of IN insurance NN that WDT covers VVZ damage NN that WDT can MD occur VV to TO other JJ people NNS . SENT PULL NN PLATES NNS . SENT Several JJ types NNS of IN special JJ plates NNS that WDT can MD be VB bolted VVN , , soldered VVN or CC braze VV welded VVN onto IN the DT damaged JJ panel NN . SENT The DT damaged JJ area NN can MD then RB be VB pulled VVN out RP by IN attaching VVG the DT hydraulic JJ jack NN to TO the DT pull NN plates NNS in IN a DT variety NN of IN pulling VVG combinations NNS . SENT PULL NN RODS NNS . SENT Rods NNS that WDT are VBP equipped VVN with IN hooks NNS on IN one CD end NN and CC handles VVZ on IN the DT other JJ . SENT The DT hooked JJ ends NNS are VBP inserted VVN into IN small JJ holes NNS drilled VVN in IN areas NNS of IN direct JJ damage NN and CC used VVN in IN roughly RB aligning VVG the DT areas NNS of IN direct JJ damage NN before IN they PP are VBP soldered VVN or CC welded VVN . SENT PUNCHES NNS . SENT Special JJ tools NNS used VVN in IN driving VVG shafts NNS and CC pins NNS and CC in IN aligning VVG holes NNS in IN panels NNS so RB that IN they PP can MD be VB bolted VVN together RB . SENT Different JJ punches NNS are VBP used VVN in IN the DT metal NN finishing VVG operation NN for IN raising VVG low JJ spots NNS located VVN around IN the DT outer JJ edges NNS of IN inaccessible JJ body NN panels NNS . SENT PUSHING VVG . SENT Hydraulic JJ jack NN set VVN up RP to TO push VV out RP collision NN damage NN . SENT PUTTY JJ GLAZING NN . SENT Heavy NP bodied VVD nitrocellulose NN or CC polyester NN material NN used VVN to TO fill VV small JJ flaws NNS that WDT are VBP in IN the DT surface NN and CC are VBP too RB large JJ to TO be VB filled VVN by IN primer JJR surfacer NN . SENT PUTTY JJ KNIFE NN . SENT Special JJ knife NN used VVN in IN applying VVG glazing NN putty NN . SENT Q NP Back RB to TO General NP Terms NNS Index NP QUARTER NN PANEL NN . SENT Side NN panel NN that WDT is VBZ generally RB a DT quarter NN of IN the DT total JJ length NN of IN the DT vehicle NN and CC extends VVZ from IN the DT rear JJ door NN to TO the DT end NN of IN the DT car NN . SENT QUARTZ NN HALOGEN NN . SENT Headlight NN system NN noted VVD for IN the DT extra JJ amount NN of IN light NN it PP gives VVZ a DT driver NN if IN the DT vehicle NN is VBZ so RB equipped VVN at IN night NN . SENT QUENCHING VVG . SENT Cooling VVG of IN a DT shrink VV spot NN or CC solder VV fill VV with IN a DT wet JJ rag NN or CC sponge NN . SENT R SYM RADIATOR NN . SENT Part NN of IN the DT vehicle NN through IN which WDT the DT coolant NN flows VVZ to TO be VB cooled VVN . SENT RAIN NN OR CC WATER NN SPOTTING VVG . SENT Marks NNS on IN the DT surface NN due JJ to TO rain NN or CC water NN absorption NN . SENT RECYCLED JJ PARTS NNS . SENT Parts NNS of IN a DT vehicle NN that WDT have VHP been VBN used VVN and CC are VBP bought VVN from IN a DT recycler NN . SENT REDUCE VV . SENT Lower JJR or CC make VV less JJR in IN consistency NN . SENT to TO cut VV . SENT REDUCER NN . SENT Referred VVN to TO as IN the DT volatile JJ substance NN used VVN to TO thin JJ the DT viscosity NN of IN enamel NN prior RB to TO application NN . SENT REFINISH NP . SENT Term NN used VVD to TO designate VV that IN a DT part NN or CC a DT vehicle NN is VBZ to TO be VB repainted VVN . SENT REFLOW NP . SENT Heat NN process NN used VVN to TO melt VV lacquer NN to TO produce VV a DT better JJR flow NN or CC leveling NN . SENT REGULATOR NN DOOR NN . SENT Mechanism NN in IN a DT door NN used VVN to TO raise VV and CC lower VV the DT glass NN . SENT RELATIVE JJ HUMIDITY NN . SENT Condition NN of IN the DT atmosphere NN with IN reference NN to TO its PP$ content NN of IN water NN vapor NN at IN a DT given VVN temperature NN . SENT RELIEVING VVG . SENT Process NN of IN removing VVG and CC correcting VVG stresses NNS in IN a DT panel NN due JJ to TO collision NN damage NN . SENT RESPIRATOR NN . SENT Filtering VVG device NN worn VVN over IN the DT mouth NN and CC nose NN to TO filter NN out IN particles NNS and CC fumes NNS and CC prevent VV them PP from IN reaching VVG the DT lungs NNS . SENT RETARDER NN . SENT Slowly RB evaporating VVG thinner JJR used VVN to TO retard VV drying VVG . SENT RETEXTURE NN . SENT To TO apply VV texture NN paint NN over IN a DT repaired VVN area NN RETRACTOR NN . SENT Mechanism NN that WDT pulls VVZ a DT safety NN belt NN back RB into IN its PP$ proper JJ place NN . SENT ROCKER NN PANELS NNS . SENT Assemblies NNS of IN box NN type NN construction NN located VVN directly RB below IN the DT doors NNS , , that WDT are VBP not RB only JJ spot NN welded VVN to TO the DT cowl NN assembly NN in IN front NN and CC to TO the DT rear JJ quarter NN panel NN assembly NN at IN the DT rear JJ but CC also RB to TO the DT side NN of IN the DT under IN body NN section NN . SENT ROLLED JJ BUCKLE NN . SENT Buckle NN created VVD by IN a DT force NN that WDT extends VVZ over IN the DT crowned VVN surface NN of IN a DT panel NN . SENT ROOF NN RAIL NN . SENT Reinforcements NNS welded VVN to TO the DT pillars NNS and CC to IN which WDT the DT roof NN panel NN is VBZ welded VVN . SENT ROSIN NN . SENT Natural JJ gum NN or CC resin NN . SENT residue NN of IN the DT distillation NN of IN crude JJ turpentine NN . SENT ROTOR NN ASSEMBLY NN . SENT Part NN of IN the DT wheel NN brake NN assembly NN to TO which WDT hydraulic JJ pressure NN is VBZ applied VVN to TO stop VV a DT vehicle NN . SENT RUBBER NN OR CC SPACER NN DAM NN . SENT Rubber NN strip NN installed VVN on IN the DT pinchweld JJ fence NN to TO prevent VV the DT adhesive NN from IN oozing VVG out RP . SENT RUBBING VVG AND CC POLISHING VVG COMPOUND NN . SENT Special JJ type NN of IN abrasive NN used VVN to TO smooth VV out RP and CC polish VV a DT paint NN film NN . SENT RUN NN SAGS NNS . SENT When WRB too RB many JJ or CC too RB heavy JJ coats NNS are VBP applied VVN at IN one CD time NN causing VVG the DT film NN to TO droop VV under IN its PP$ own JJ weight NN . SENT S PP Back RB to TO General NP Terms NNS Index NP SAG NN . SENT Type NN of IN frame NN damage NN in IN which WDT one PP or CC both DT side NN rails VVZ bend VV and CC sag VV at IN the DT cowl NN causing VVG buckles NNS to TO be VB formed VVN on IN the DT top NN of IN the DT side NN rails VVZ . SENT SAND NN SCRATCH NN SWELLING VVG . SENT exaggerated JJ reproduction NN and CC distortion NN of IN the DT sanding VVG marks NNS in IN the DT underlying JJ surface NN . SENT SAND NN SCRATCHES NNS . SENT Reproduction NN in IN the DT topcoat NN of IN the DT sanding VVG marks NNS in IN the DT underlying JJ surface NN . SENT SANDBLASTER NN . SENT Piece NN of IN equipment NN used VVN to TO clean VV metal NN using VVG sand NN and CC pressurized VVN air NN . SENT SANDER JJR . SENT Power NP driven JJ tool NN used VVN with IN abrasives NNS to TO sand NN car NN bodies NNS . SENT SANDER JJR POLISHER NN . SENT Power NN tool NN used VVN to TO speed VV up RP the DT rate NN of IN polishing VVG or CC sanding VVG surfaces NNS . SENT SANDING VVG BLOCK NN . SENT Hard JJ rubber NN or CC plastic JJ flexible JJ block NN used VVN to TO provide VV consistent JJ backing NN for IN hand NN sanding VVG . SENT SATURATION NN . SENT Refers VVZ to TO a DT color's JJ purity NN and CC richness NN . SENT SCUFF NN SAND NN . SENT To TO lightly RB sand NN a DT surface NN with IN an DT abrasive JJ pad NN . SENT SEALER NN . SENT Paint NN product NN used VVN to TO prevent VV bleed VV through RP of IN the DT previous JJ coat NN or CC the DT sinking NN in IN of IN the DT new JJ paint NN , , resulting VVG in IN loss NN of IN gloss VV . SENT SECTIONING VVG . SENT Process NN of IN joining VVG two CD different JJ sections NNS of IN a DT part NN or CC vehicle NN by IN welding VVG to TO make VV one CD part NN , , SEEDINESS NN . SENT Being VBG gritty JJ or CC sandy JJ or CC full JJ of IN small JJ grains NNS . SENT SELF NN CENTERING VVG GAUGE NN . SENT Gauge NN used VVD in IN frame NN repair NN that IN centers NNS at IN all DT times NNS as IN it PP is VBZ pulled VVN out RP or CC pushed VVD out RP . SENT SEPARATION NN . SENT Non JJ uniform JJ mixture NN . SENT SERIES NN CIRCUIT NN . SENT Circuit NN through IN which WDT current JJ flows NNS in IN an DT angle NN continuous JJ path NN . SENT SERRATED JJ SADDLE NN . SENT Attachment NN used VVD to TO protect VV the DT threads NNS on IN the DT extension NN tubing NN and CC the DT ram NN plunger NN . SENT Its PP$ serrated JJ face NN serves VVZ as IN a DT base NN that IN doesn't JJ slip NN or CC slide VV easily RB when WRB pressure NN is VBZ applied VVN . SENT SET VVN BACK RB . SENT Term NN used VVD to TO indicate VV that IN one CD of IN the DT front JJ wheels NNS is VBZ farther RB back RB than IN the DT other JJ . SENT SETTING VVG UP RP . SENT Period NN during IN which WDT solvent JJ evaporation NN from IN the DT film NN flowing JJ ceases VVZ and CC the DT film NN surface NN becomes VVZ tack NN free JJ . SENT SHADE NN . SENT Variation NN of IN a DT color NN . SENT Assuming VVG that IN a DT color NN is VBZ generally RB blue JJ , , it PP can MD have VH a DT red JJ shade NN or CC a DT yellow JJ shade NN as IN well RB as IN being VBG blue JJ . SENT Shade NN is VBZ also RB called VVN undertone NN since IN it PP describes VVZ the DT subtle JJ tone NN of IN a DT color NN . SENT SHAPE NN . SENT Form NN to TO which WDT a DT metal NN panel NN was VBD stamped VVN . SENT SHIFTING VVG LINKAGE NN CABLE NN . SENT Cable NP used VVD to TO shift VV the DT gears VVZ in IN a DT vehicle NN . SENT SHOCK NN ABSORBER NN . SENT Mechanism NN that WDT uses VVZ fluid JJ , , pistons NNS , , and CC valves NNS to TO dampen VV the DT oscillation NN of IN a DT vehicle NN . SENT SHORT JJ CIRCUIT NN . SENT Current JJ that IN flows NNS in IN a DT continuous JJ path NN that WDT bypasses VVZ a DT portion NN of IN its PP$ intended JJ circuit NN , , usually RB directly RB to TO ground NN or CC into IN another DT circuit NN . SENT SHRINKAGE NN . SENT Operation NN by IN means NNS of IN which WDT stretched VVD areas NNS on IN damaged JJ auto NN body NN parts NNS and CC panels NNS are VBP disposed VVN of IN and CC brought VVD back RB to TO their PP$ original JJ shape NN and CC size NN . SENT SHROUD NN . SENT Sheet NN metal NN or CC plastic NN part NN used VVN on IN cars NNS to TO direct VV the DT flow NN of IN cooling VVG air NN . SENT SILICON NN CARBIDE NN . SENT Abrasive NN made VVD by IN fusing VVG silica NN and CC coke NN in IN an DT electric JJ furnace NN . SENT The DT abrasive NN is VBZ very RB hard JJ , , shiny JJ black JJ and CC iridescent JJ . SENT SIMPLE JJ HINGE NN BUCKLE NN . SENT Formed VVN when WRB flat JJ sheet NN metal NN is VBZ forced VVN to TO bend VV either RB inward RB or CC outward RB by IN a DT damaging JJ force NN or CC impact NN . SENT It PP is VBZ similar JJ to TO the DT bending VVG of IN a DT hinge NN on IN a DT door NN and CC the DT change NN in IN the DT grain NN or CC molecular JJ structure NN of IN the DT metal NN that WDT occurs VVZ will MD vary VV greatly RB , , depending VVG on IN the DT sharpness NN of IN the DT bend VV . SENT SIMPLE JJ ROLLED JJ BUCKLE NN . SENT Outer JJ ridges NNS formed VVN at IN either DT end NN of IN a DT hinge NN buckle NN that WDT extends VVZ or CC crosses VVZ over RP into IN the DT crowned VVN surface NN of IN auto NN body NN panel NN . SENT SINGLE JJ COAT NN . SENT Usually RB referred VVN to TO as IN a DT coat NN of IN paint NN . SENT Once RB over IN the DT surface NN with IN each DT stroke NN overlapping VVG the DT previous JJ stroke NN 50 CD percent NN . SENT SINGLE JJ STAGE NN COMPRESSOR NN . SENT Compressor NN in IN which WDT atmospheric JJ air NN pressure NN is VBZ compressed VVN to TO container NN pressure NN in IN one CD operation NN . SENT SINKING VVG IN IN . SENT Term NN applied VVD when WRB one CD coat NN is VBZ partially RB absorbed VVN by IN the DT previous JJ one NN . SENT SKINNING VVG . SENT Oxidation NN , , hardening VVG or CC drying VVG of IN a DT paint NN at IN the DT surface NN of IN the DT liquid JJ while NN in IN its PP$ container NN . SENT SLIDE NN HAMMER NN . SENT Weight NN that IN slides NNS along IN a DT bar NN until IN it PP hits VVZ a DT stop NN . SENT The DT bar NN usually RB has VHZ attachments NNS to TO pull VV dents NNS out RP , , and CC the DT impact NN that IN results NNS when WRB the DT weight NN hits VVZ the DT stop NN helps VVZ to TO pull VV the DT dent NN out RP . SENT SMC NP SHEET NN MOLDED VVN COMPOUND NN . SENT Fiber NN plastic NN type NN of IN material NN that WDT is VBZ molded VVN to TO a DT certain JJ form NN and CC used VVN as IN an DT outer JJ panel NN on IN a DT vehicle NN . SENT SMEC NP SINGLE JJ MODULE NN ENGINE NN CONTROLLER NN . SENT Computer NN module NN that WDT controls VVZ the DT functions NNS of IN the DT various JJ components NNS of IN the DT power NN train NN . SENT SOLDER NN . SENT Mixture NN of IN lead NN and CC tin NN used VVN to TO fill VV dents NNS and CC joints NNS on IN body NN panels NNS . SENT SOLDERING VVG SALTS NNS . SENT Non JJ acid JJ flux NN employed VVN in IN the DT tinning VVG of IN metal NN . SENT SOLIDS NNS . SENT Part NN of IN the DT paint NN that WDT does VVZ not RB evaporate VV and CC stays VVZ on IN the DT surface NN . SENT SOLUTION NN . SENT Homogeneous JJ liquid NN or CC mixture NN of IN two CD or CC more JJR chemical NN substances NNS . SENT SOLVENCY NN . SENT Ability NN or CC power NN of IN causing VVG solution NN . SENT Ability NN to TO dissolve VV . SENT SOLVENT JJ . SENT Any DT liquid NN in IN or CC by IN which WDT a DT substance NN can MD be VB dissolved VVN . SENT SOLVENT JJ POPPING VVG . SENT Blisters NNS that IN form NN on IN a DT paint NN film NN caused VVN by IN trapped JJ solvents NNS . SENT SPECIFIC JJ GRAVITY NN . SENT Weight NN of IN a DT certain JJ amount NN of IN liquid NN compared VVN to TO the DT same JJ amount NN of IN water NN at IN the DT same JJ constant JJ temperature NN . SENT SPEED NN FILE NN . SENT Special JJ file NN that WDT has VHZ a DT straight JJ solid JJ base NN about IN 2 CD inches NNS wide JJ and CC 17 CD inches NNS long JJ onto IN which WDT strips NNS of IN sandpaper NN are VBP fastened VVN . SENT This DT file NN is VBZ used VVN in IN sanding VVG down RP solder NN and CC plastic JJ filled VVN areas NNS to TO their PP$ final JJ shape NN and CC contour NN . SENT SPIRIT NN LEVEL NN . SENT Instrument NN used VVD to TO find VV if IN an DT item NN is VBZ level NN . SENT SPLICE NN CLIP NN . SENT Joint NP used VVD to TO join VV two CD or CC three CD pieces NNS of IN wire NN . SENT SPOON NN . SENT Tool NN that WDT is VBZ designed VVN to TO perform VV the DT same JJ work NN as IN a DT dolly NN , , but CC is VBZ thin JJ , , wide JJ , , and CC fairly RB long JJ and CC can MD be VB used VVN in IN areas NNS that WDT have VHP very RB little JJ clearance NN . SENT SPOT NN OR CC PLUG VV WELDING VVG . SENT Weld NP made VVD through IN a DT hole NN in IN a DT panel NN . SENT SPOT NN REPAIR NN . SENT Small JJ refinish JJ repair NN job NN in IN which WDT a DT small JJ section NN of IN a DT panel NN is VBZ refinished JJ . SENT SPRAY NN BOOTH NN . SENT Enclosure NN used VVD to TO paint VV a DT vehicle NN that WDT has VHZ air NN moving VVG through IN it PP . SENT SPRAY NN GUN NN . SENT Device NN that WDT mixes VVZ paint NN and CC compressed VVN air NN to TO atomize VV and CC control VV the DT spray NN pattern NN as IN the DT paint NN leaves VVZ the DT fluid JJ needle NN and CC cap NN . SENT SPREADER JJR ADJUSTMENT NN VALVE NN . SENT Valve NN in IN a DT spray NN gun NN that WDT adjusts VVZ the DT spray NN pattern NN . SENT SPREADER JJR TOES NNS . SENT Attachments NNS designed VVN to TO anchor VV combinations NNS against IN frame NN members NNS , , braces NNS , , and CC the DT heads NNS of IN body NN bolts NNS . SENT SPRING NN HAMMERING NN . SENT Elimination NN of IN a DT high JJ ridges NNS generally RB formed VVN at IN the DT outer JJ edges NNS of IN indirect JJ damage NN by IN means NNS of IN hammering VVG them PP down RP with IN a DT surfacing VVG spoon NN and CC bumping VVG hammer NN . SENT SPRINGBACK NP . SENT Amount NN that IN a DT section NN of IN a DT vehicle NN will MD move VV back RB once IN the DT hydraulic JJ pressure NN is VBZ removed VVN . SENT SQUARING VVG . SENT Operating VVG of IN straightening VVG a DT damaged JJ section NN and CC equalizing VVG the DT diagonal JJ measurements NNS to TO bring VV the DT section NN back RB to TO specifications NNS . SENT SQUEEGEE NN . SENT Rectangular JJ piece NN of IN rubber NN approx NN . SENT 2 CD inches NNS wide JJ and CC 3 CD inches NNS long RB . SENT It PP is VBZ used VVN in IN applying VVG glazing NN putty NN and CC filler NN on IN concave JJ surfaces NNS . SENT STARTER NN . SENT Electric JJ motor NN used VVN to TO turn VV the DT engine NN to TO start VV it PP . SENT STATE NN . SENT To TO remove VV the DT stresses NNS accumulated VVN when WRB distorted VVN by IN a DT collision NN and CC completely RB relieved VVN . SENT STATIC JJ BALANCE NN . SENT Condition NN in IN which WDT a DT wheel NN and CC tire NN can MD be VB rotated VVD and CC the DT assembly NN will MD not RB stop VV at IN the DT same JJ place NN after IN each DT rotation NN . SENT STATIC JJ LOAD NN . SENT Load NN that WDT is VBZ exerted VVN by IN the DT weight NN of IN the DT vehicle NN and CC the DT frame NN members NNS , , at IN rest NN . SENT STEEL NN MUSIC NN WIRE NN . SENT Wire NN used VVD in IN a DT piano NN that WDT can MD be VB used VVN as IN a DT cutting VVG edge NN to TO cut VV adhesive NN . SENT STEERING VVG AXLE NN INCLINIATION NN . SENT Inward RB tilt VV of IN the DT king NN pin NN or CC spindle NN support NN arm NN at IN the DT top NN . SENT It PP is VBZ a DT directional JJ control NN angle NN measured VVN in IN degrees NNS and CC is VBZ the DT amount NN the DT spindle NN support NN center NN line NN is VBZ tilted VVN from IN the DT true JJ vertical JJ . SENT STEERING NN COLUMN NN . SENT Mechanism NN used VVD to TO steer VV the DT vehicle NN . SENT STRAIGHT JJ LINE NN SANDER NN . SENT Sander NN that WDT uses VVZ a DT back RB and CC forth RB movement NN to TO sand NN a DT surface NN using VVG sandpaper NN on IN its PP$ shoe NN . SENT STRAIGHT JJ TIME NN . SENT Timing VVG an DT operation NN by IN the DT elapsed VVN time NN as RB punched VVD in IN on IN a DT clock NN . SENT STRENGTH NN . SENT Amount NN of IN pigment NN . SENT High JJ strength NN bases NNS contain VVP a DT lot NN of IN pigment NN . SENT The DT additional JJ pigment NN gives VVZ the DT bases NNS good JJ hiding NN . SENT STRESS NN . SENT Amount NN of IN pressure NN that WDT is VBZ applied VVN to TO a DT piece NN of IN metal NN when WRB it PP is VBZ bent JJ and CC the DT metal NN cannot NN return NN to TO its PP$ original JJ shape NN . SENT STRETCHED VVN . SENT Amount NN by IN which WDT a DT metal NN surface NN has VHZ become VVN larger JJR or CC longer JJR . SENT STRIKER NN PLATE NN OR CC BOLT NN . SENT Part NN that WDT is VBZ installed VVN on IN the DT door NN frame NN in IN which WDT the DT lock NN engages VVZ to TO lock VV the DT door NN . SENT STRIP VV CAULKING VVG . SENT Sealer NN sold VVD in IN the DT shape NN of IN a DT strip NN . SENT STROKING VVG . SENT Motion NN used VVD when WRB painting NN with IN a DT spray NN gun NN . SENT STRUCTURAL JJ ADHESIVE NN . SENT Adhesive NN used VVD to TO repair VV the DT structure NN of IN a DT plastic JJ part NN such JJ as IN a DT bumper NN cover NN . SENT SUB NN ASSEMBLY NN . SENT An DT assembly NN within IN a DT multi NNS level NN assembly NN that WDT is VBZ available JJ individually RB from IN the DT vehicle NN manufacturer NN . SENT SUBLET VV . SENT To TO let VV work NN that IN one CD has VHZ contracted VVN to TO do VV to TO a DT subordinate JJ contractor NN . SENT SUBLET VV REPAIRS NNS . SENT Repairs NNS to TO be VB performed VVN for IN a DT negotiated VVN or CC contract NN price NN , , or CC by IN a DT subcontractor NN . SENT All DT applicable JJ materials NNS , , labor NN , , markup NN , , and CC taxes NNS should MD be VB included VVN when WRB a DT Sublet VV Repair NP is VBZ indicated VVN . SENT SUBSTRATE NN . SENT Surface VV to TO be VB painted VVN whether IN an DT old JJ finish NN or CC bare JJ metal NN . SENT SUCTION NN FEED NN GUN NN . SENT Spray NN gun NN that WDT has VHZ the DT paint NN container NN connected VVN directly RB to TO it PP . SENT It PP is VBZ designed VVN to TO create VV a DT vacuum NN and CC thus RB draw VV the DT paint NN from IN the DT container NN . SENT SUN NN ROOF NN PANEL NN . SENT Panel NN in IN the DT roof NN panel NN of IN a DT vehicle NN which WDT can MD be VB raised VVN up RP slightly RB or CC slid VVD back RB in IN the DT opening NN to TO let VV the DT sun NN rays NNS enter VVP the DT vehicle NN . SENT SUPPLEMENT NN . SENT A DT Supplement NN is VBZ created VVN if IN a DT change NN or CC addition NN must MD be VB made VVN to TO an DT estimate NN where WRB a DT final JJ print NN has VHZ been VBN produced VVN . SENT SURFACE VV DRYING VVG . SENT Drying VVG of IN the DT topcoat NN while IN the DT bottom JJ coats NNS have VHP remained VVN soft JJ . SENT SWEATING VVG . SENT Separation NN and CC appearance NN at IN the DT film NN surface NN of IN the DT oil NN in IN lacquer NN . SENT SYMMETRICAL JJ . SENT Regular JJ well RB balanced JJ arrangement NN of IN parts NNS and CC opposite JJ sides NNS of IN a DT line NN or CC plain JJ or CC around IN a DT center NN axis NN . SENT SYNTHETIC JJ RESIN NN . SENT Any DT resin NN not RB produced VVN by IN nature NN . SENT manmade JJ . SENT T NN Back RB to TO General NP Terms NNS Index NP TACK NN COAT NN . SENT The DT first JJ enamel NN coat NN . SENT A DT full JJ coat NN that WDT is VBZ to TO dry VV only RB until IN it PP is VBZ quite RB sticky JJ . SENT TACK NN RAG NN . SENT Cloth NN impregnated VVD with IN varnish NN . SENT used VVN as IN a DT final JJ cleanup NN to TO remove VV dust NN before IN applying VVG the DT finishing JJ paint NN . SENT TACK NN WELDS VVZ . SENT Short RB welds VVZ placed VVN at IN intervals NNS along IN a DT break NN or CC the DT joining VVG edges NNS of IN two CD pieces NNS of IN metal NN , , keeping VVG the DT metal NN in IN alignment NN while IN the DT bead NN is VBZ run VVN . SENT TACK NN FREE JJ . SENT That DT point NN of IN time NN in IN drying VVG at IN which WDT the DT surface NN of IN the DT film NN will MD not RB fingerprint NN . SENT yet RB the DT film NN is VBZ not RB dry JJ and CC hard RB throughout IN . SENT TEE NN WELD NN . SENT Welding NP procedure NN that WDT forms VVZ a DT T NN . SENT TEMPLATE NN . SENT Pattern NN made VVD from IN a DT part NN so RB that IN another DT part NN can MD be VB made VVN to TO the DT exact JJ same JJ shape NN . SENT TENSILE JJ STRENGTH NN . SENT Amount NN of IN axial JJ elongation NN pressure NN that WDT can MD be VB exerted VVN on IN a DT material NN before IN it PP begins VVZ to TO deform VV . SENT TENSION NN PLATES NNS . SENT Metal NN plates NNS used VVN to TO pull VV damaged JJ metal NN back RB to TO its PP$ former JJ shape NN . SENT fastened VVN to TO the DT metal NN surface NN by IN using VVG solder NN or CC plastic NN filler NN . SENT TEST NN LIGHT NN . SENT Usually RB , , a DT light NN used VVN to TO check VV for IN voltage NN or CC current JJ in IN a DT circuit NN to TO locate VV open JJ conditions NNS . SENT the DT ground NN cable NN back RB to TO the DT welding VVG machine NN . SENT THERMOPLASTIC NN . SENT Type NN of IN plastic NN that WDT can MD be VB softened VVN with IN the DT application NN of IN heat NN , , can MD be VB reshaped VVN , , and CC can MD also RB be VB welded VVN . SENT THERMOPLASTIC JJ POLYURETHANE NN . SENT Plastic NN that WDT can MD be VB softened VVN by IN applying VVG heat NN , , reshaped VVN and CC welded VVN . SENT THERMOSETTING JJ . SENT Type NN of IN plastic NN that WDT is VBZ permanently RB set VVN . SENT It PP can't NN be VB softened VVN with IN heat NN or CC reshaped VVN or CC welded VVN . SENT Minor JJ damage NN can MD often RB be VB repaired VVN with IN a DT structural JJ adhesive NN . SENT THERMOSTAT NN . SENT Mechanism NN used VVD to TO control VV heat NN . SENT THICKNESS NN OF IN FILM NN . SENT Measurement NN of IN a DT film NN usually RB expressed VVD in IN mils NNS of IN the DT distance NN from IN top NN to TO bottom NN or CC at IN right JJ angles NNS to TO its PP$ surface NN . SENT THINNER JJR . SENT Commonly RB known VVN as IN a DT lacquer NN solvent JJ , , which WDT reduces VVZ the DT viscosity NN of IN a DT lacquer NN to TO spraying VVG consistency NN . SENT TIE NN RODS NNS . SENT Rod NN like IN component NN of IN the DT steering NN linkage NN composed VVN of IN strong JJ steel NN tubing NN that WDT links VVZ a DT steering VVG arm NN to TO the DT center NN link NN . SENT TINNING VVG . SENT Process NN of IN applying VVG a DT thin JJ coat NN of IN material NN to TO metal NN to TO improve VV adherence NN . SENT TINT NN . SENT Mixture NN of IN two CD or CC more JJR pigments NNS . SENT TINTING VVG COLOR NN . SENT Finishing VVG lacquer NN or CC enamel NN in IN which WDT only RB one CD pigment NN or CC color NN is VBZ normally RB used VVN . SENT TOE NN IN IN . SENT Distance VV the DT front NN of IN the DT front JJ wheels NNS is VBZ closer RBR together RB than IN the DT rear NN of IN the DT front JJ wheels NNS . SENT TOOTH NN . SENT Roughened VVN surface NN that WDT affects VVZ adhesion NN of IN the DT coating NN . SENT TOPCOAT NN . SENT Last JJ of IN final JJ color NN coat NN . SENT TORQUE NN ROD NN . SENT Type NN of IN a DT spring NN used VVN to TO help VV open VV and CC counteract VV the DT weight NN of IN the DT trunk NN lid NN . SENT TORQUE NN STEER VV . SENT Condition NN in IN some DT front JJ wheel NN drive NN vehicles NNS wherein RB more JJR torque NN is VBZ applied VVN to TO one CD wheel NN than IN the DT other JJ . SENT TOW RB , , FIRST NP . SENT Accident NN tow NN . SENT TOXICITY NN . SENT Pertaining VVG to TO poisonous JJ effect NN . SENT TRACKING VVG . SENT When WRB the DT rear JJ wheels NNS of IN a DT vehicle NN follow VV the DT front JJ wheels NNS evenly RB on IN each DT side NN . SENT TRAM NN GAUGES VVZ . SENT Gauges VVZ used VVN to TO accurately RB measure VV and CC diagnose VV body NN and CC frame NN collision NN damages NNS for IN all DT conventional JJ and CC unitized JJ vehicles NNS . SENT TRANSAXLE NP . SENT Drive NN system NN used VVN mainly RB on IN front JJ wheel NN drive NN vehicles NNS . SENT TRANSFORMER NN . SENT Equipment NN used VVD to TO regulate VV and CC clean VV air NN used VVN to TO paint VV vehicles NNS . SENT TRANSPARENT JJ . SENT Bases NNS that WDT contain VVP a DT small JJ amount NN of IN pigment NN . SENT You PP can MD see VV through IN the DT base NN . SENT TRICOAT NP PAINT NN JOB NN . SENT Paint NN system NN that WDT uses VVZ a DT base JJ color NN coat NN then RB a DT pearl NN luster VV coat NN , , followed VVN by IN a DT clearcoat NN . SENT TRIGGERING VVG . SENT Procedure NN used VVD on IN a DT spray NN gun NN to TO move VV the DT trigger NN . SENT TRUNK NN LID NN . SENT Panel NN used VVD to TO close VV the DT open JJ area NN between IN the DT quarter NN panels NNS . SENT TURNING VVG RADIUS NN . SENT Tire NN wearing VVG angle NN measured VVN in IN degrees NNS . SENT The DT amount NN one CD front NN wheel NN turns VVZ more RBR sharply RB than IN the DT other JJ wheel NN does VVZ on IN turns NNS . SENT TURRET NN TOP NN . SENT Part NN of IN the DT vehicle NN that WDT covers VVZ the DT passenger NN compartment NN . SENT TWIST NN . SENT Type NN of IN frame NN damage NN in IN which WDT both DT side NN rails NNS are VBP bent JJ out RB of IN alignment NN , , so RB that IN they PP do VVP not RB run VV horizontally RB parallel JJ to TO one CD another DT . SENT TWO CD COMPONENT NN SYSTEM NN . SENT Materials NNS such JJ as IN some DT paints NNS , , fillers NNS , , and CC adhesives NNS that WDT require VVP the DT addition NN of IN an DT additive NN to TO accomplish VV a DT chemical JJ reaction NN causing VVG it PP to TO harden VV . SENT TWO CD STAGE NN COMPRESSOR NN . SENT Compressor NN that WDT compresses VVZ air NN to TO cylinder NN pressure NN in IN two CD stages NNS using VVG two CD cylinders NNS . SENT TWO CD TONE NN . SENT Two CD different JJ colors NNS used VVN on IN a DT single JJ paint NN job NN . SENT U NP Back RB to TO General NP Terms NNS Index NP UHSS NP ULTRAHIGH NP STRENGTH NN STEEL NN . SENT Very RB high JJ strength NN steel NN which WDT is VBZ used VVN for IN parts NNS such JJ as IN door NN guard NN beams VVZ . SENT UNDERCOAT NN . SENT Material NN used VVD to TO protect VV the DT underbody NN sections NNS of IN a DT vehicle NN . SENT UNITIZED JJ BODY NN CONSTRUCTION NN . SENT Construction NN in IN which WDT the DT frame NN and CC body NN are VBP made VVN out RP of IN a DT large JJ number NN of IN sheetmetal JJ panels NNS of IN varying VVG sizes NNS and CC shapes NNS assembled VVN and CC welded VVN into IN a DT single JJ unit NN . SENT UNLOCKING VVG THE DT METAL NN . SENT Unfolding VVG and CC reshaping VVG of IN the DT V NN channels NNS , , valleys NNS and CC buckles NNS as IN gently RB as RB possible JJ , , without IN further RBR stretching VVG , , creasing VVG or CC upsetting VVG the DT metal NN . SENT UPPER JJ RAIL NN . SENT Part NN used VVD on IN top NN of IN the DT shield NN to TO increase VV the DT strength NN of IN the DT front JJ section NN . SENT UPSETTING VVG . SENT Application NN of IN heat NN on IN metal NN that WDT is VBZ restricted VVN from IN expanding VVG in IN all DT directions NNS and CC yet RB allowed VVN to TO contract NN in IN all DT directions NNS when WRB it PP cools VVZ . SENT URETHANE NN ADHESIVE NN . SENT Plastic JJ type NN of IN adhesive NN . SENT USED VVN CLIP NN . SENT Section NN of IN a DT vehicle NN purchased VVN from IN a DT recycler NN and CC welded VVN or CC bolted VVN to TO a DT vehicle NN . SENT V NN Back RB to TO General NP Terms NNS Index NP VACUUM NN PUMP NN . SENT Pump NN that WDT creates VVZ a DT vacuum NN condition NN , , such JJ as IN on IN air NN conditioning NN systems NNS . SENT VANDALIZED VVD . SENT Intentional JJ damage NN to TO a DT vehicle NN . SENT VAPORIZATION NN . SENT Process NN of IN solvent JJ evaporation NN . SENT VEHICLE NN . SENT Liquid JJ portion NN of IN a DT paint NN . SENT VINYL NN COATED JJ FABRIC NN . SENT Fabric NN coated VVN with IN vinyl NN material NN . SENT VINYL NN GUARD NN . SENT Vinyl NN paint NN applied VVN to TO the DT lower JJR portion NN of IN an DT automobile NN to TO protect VV it PP from IN stone NN bruises NNS . SENT VINYL NN CLAD JJ URETHANE NN FOAM NN . SENT Combinations NNS of IN these DT materials NNS used VVN as IN padding NN on IN such JJ items NNS as IN the DT crash NN pad NN on IN a DT dash NN . SENT VISCOSITY NN . SENT Thickness NN of IN a DT fluid NN . SENT resistance NN to TO flow VV . SENT VOLATILE JJ . SENT Capable JJ of IN evaporating VVG easily RB . SENT an DT area NN that WDT readily RB vaporizes VVZ VOLTMETER NN . SENT Electronic JJ meter NN used VVN to TO measure VV voltage NN . SENT W NP Back RB to TO General NP Terms NNS Index NP WADDLE VV . SENT Condition NN caused VVD by IN some DT defective JJ radial JJ tires NNS which WDT cause VVP the DT vehicle NN to TO have VH sideways RB back RB and CC forth RB motion NN due JJ to TO broken JJ or CC defective JJ belts NNS . SENT WATER NN SPOTTING VVG . SENT Condition NN caused VVD by IN water NN evaporating VVG on IN a DT paint NN film NN before IN it PP is VBZ thoroughly RB dry JJ resulting VVG in IN a DT dulling VVG of IN the DT gloss VVP in IN spots NNS . SENT WEATHERING NN . SENT Change NN or CC failure NN in IN paint NN caused VVN by IN exposure NN to TO the DT weather NN . SENT WELDING VVG . SENT Process NN of IN joining VVG two CD pieces NNS of IN metal NN to TO form VV a DT single JJ piece NN of IN metal NN . SENT WET JJ SANDING VVG . SENT Procedure NN of IN sanding VVG paint NN film NN with IN sandpaper NN and CC water NN . SENT WET JJ SPOTS NNS . SENT Discoloration NN caused VVD where WRB the DT paint NN fails VVZ to TO dry VV and CC adhere VV uniformly RB . SENT caused VVN by IN grease NN or CC finger NN marks NNS usually RB . SENT WHEEL NN ALIGNMENT NN . SENT Procedure NN of IN aligning VVG wheels NNS to TO the DT manufacturer's JJ specifications NNS . SENT WHEEL NN BALANCING NN . SENT Proper JJ distribution NN of IN weight NN around IN a DT tire NN and CC wheel NN assembly NN to TO counteract VV centrifugal JJ forces NNS acting VVG upon IN the DT heavy JJ areas NNS in IN order NN to TO maintain VV a DT true JJ running VVG wheel NN perpendicular NN to TO its PP$ rotating VVG axis NN . SENT WHEELHOUSES NNS . SENT Deep RB curved VVN panels NNS that WDT form VVP the DT compartments NNS in IN which WDT the DT wheels NNS rotate VV . SENT They PP are VBP generally RB bolted VVN to TO the DT front JJ fenders NNS and CC spot NN welded VVN to TO the DT rear JJ quarter NN panels NNS . SENT WINDSHIELD NN . SENT Glass NP installed VVD on IN the DT front NN of IN a DT vehicle NN to TO protect VV the DT occupants NNS from IN the DT elements NNS . SENT WINDSHIELD NN HEADER NN BAR NN . SENT Reinforcement NN by IN which WDT the DT windshield NN is VBZ supported VVN and CC to IN which WDT the DT roof NN panel NN is VBZ welded VVN . SENT WOODGRAIN NN TRANSFER NN . SENT Plastic JJ film NN that WDT has VHZ adhesive NN on IN one CD side NN and CC a DT wood NN grain NN effect NN printed VVN on IN the DT other JJ side NN , , applied VVN to TO some DT motor NN vehicles NNS . SENT WORK NN HARDENING NN . SENT Process NN of IN metal NN being VBG made VVN harder JJR by IN rolling VVG or CC hammering VVG the DT material NN . SENT WRINKLING VVG . SENT Term NN used VVD when WRB a DT paint NN film NN buckles VVZ at IN its PP$ surface NN causing VVG a DT shriveled VVD appearance NN . SENT Y NP Back RB to TO General NP Terms NNS Index NP YIELD NN STRENGTH NN . SENT Resistance NN a DT particular JJ type NN of IN material NN possesses VVZ to TO permanent JJ stretching VVG . SENT Z SYM ZIRCONIA NN . SENT Very RB rugged JJ synthetic JJ abrasive NN that WDT is VBZ used VVN mainly RB for IN rough JJ cutting NN . SENT ZONE NN SYSTEM NN . SENT Method NN of IN using VVG a DT series NN of IN zones NNS to TO enable VV writing VVG an DT accurate JJ estimate NN . SENT Unibody NN Terms NNS A DT B NP C NP D NP I NP K NP M NP P NN R NP S NP U NP Back RB to TO Top JJ A DT ACCESS NN OPENING NN . SENT The DT process NN of IN cutting VVG an DT opening NN or CC hole NN in IN the DT back JJ side NN of IN a DT panel NN or CC rail NN to TO gain VV access NN to TO a DT buckle NN or CC deformation NN in IN the DT metal NN for IN repair NN purposes NNS . SENT ANALYZE VV REPAIR NN PROCEDURES NNS . SENT The DT process NN of IN using VVG the DT information NN from IN the DT measurements NNS obtained VVD as RB well RB as IN the DT information NN from IN a DT visual JJ inspection NN to TO formulate VV a DT repair NN plan NN in IN which WDT the DT structural JJ integrity NN will MD be VB restored VVN to TO the DT vehicle NN . SENT B SYM BEND VV . SENT Damage NN to TO a DT frame NN rail NN or CC structural JJ component NN in IN which WDT the DT component NN is VBZ out RP of IN correct JJ dimensional JJ specification NN but CC is VBZ not RB severely RB weakened VVN . SENT The DT damage NN to TO a DT component NN has VHZ no DT sharp JJ edges NNS on IN the DT damage NN and CC forms VVZ a DT smooth JJ transition NN from IN the DT undamaged JJ area NN to TO the DT damaged JJ area NN . SENT A DT bend NN can MD normally RB be VB repaired VVN without IN any DT permanent JJ deformation NN to TO the DT metal NN . SENT BODY NN TWIST NN . SENT A DT condition NN to TO a DT unibody NN in IN which WDT the DT datum NN plane NN of IN the DT vehicle NN is VBZ out RP of IN specifications NNS from IN side NN to TO side NN and CC front NN to TO rear NN . SENT An DT example NN of IN this DT type NN of IN damage NN is VBZ if IN a DT vehicle NN is VBZ high JJ in IN the DT left JJ front NN , , low JJ in IN the DT right JJ rear NN and CC the DT rocker NN panels NNS are VBP not RB parallel JJ to TO each DT other JJ . SENT BUCKLE VV . SENT A DT condition NN to TO a DT frame NN rail NN , , reinforcement NN or CC apron NN from IN which WDT a DT visible JJ compression NN from IN stress NN is VBZ evident JJ . SENT C SYM Back RB to TO Unibody NP Terms NNS Index NP CENTERLINE NP BOW NN . SENT A DT condition NN in IN which WDT the DT center NN section NN is VBZ out RP of IN tolerance NN to TO the DT vehicle NN center NN line NN . SENT It PP is VBZ normally RB due JJ to TO a DT hard JJ impact NN to TO the DT side NN of IN the DT vehicle NN . SENT This DT condition NN has VHZ often RB been VBN referred VVN to TO as IN banana NN . SENT CONTROLLED VVN DIMENSIONING VVG . SENT The DT process NN of IN aligning VVG a DT suspension NN mounting VVG point NN , , arm NN or CC other JJ control NN point NN or CC bracket NN which WDT may MD not RB be VB a DT part NN of IN the DT actual JJ frame NN rail NN but CC is VBZ crucial JJ to TO proper JJ wheel NN or CC body NN alignment NN . SENT COSMETIC JJ RESTORATION NN . SENT The DT process NN of IN restoring VVG the DT factory NN appearance NN to TO a DT repaired VVN rail NN , , apron NN , , pillar NN , , rocker NN panel NN or CC other JJ structural JJ component NN . SENT Also RB is VBZ used VVN to TO describe VV the DT repairs NNS to TO a DT spliced VVN rail NN or CC component NN that WDT hide VV the DT splice NN or CC seam NN to TO return VV the DT component NN to TO a DT factory NN type NN appearance NN . SENT D SYM DIAGNOSE VV DAMAGE NN . SENT The DT process NN of IN actually RB measuring VVG the DT control NN points NNS of IN a DT damaged JJ vehicle NN and CC determining VVG which WDT ones NNS are VBP not RB dimensionally RB correct JJ . SENT DIMENSIONAL JJ PULL NN FOR IN STRUCTURAL JJ REPLACEMENT NN . SENT The DT dimensional JJ correction NN to TO a DT structural JJ member NN prior RB to TO the DT replacement NN of IN that DT member NN . SENT It PP has VHZ sometimes RB been VBN referred VVN to TO as IN a DT pre NP pull VV or CC pull VV prior RB to TO replacement NN . SENT DIRECT JJ SECONDARY JJ DAMAGE NN . SENT A DT condition NN to TO a DT firewall NN , , floor NN pan NN or CC other JJ similar JJ component NN in IN which WDT the DT component NN is VBZ pushed VVN back RB due JJ to TO an DT impact NN to TO a DT frame NN rail NN or CC apron NN . SENT The DT damage NN is VBZ a DT result NN of IN the DT impact NN to TO another DT component NN that WDT was VBD directly RB hit VVN in IN the DT collision NN . SENT This DT type NN of IN damage NN generally RB occurs VVZ to TO parts NNS that WDT are VBP welded VVN or CC joined VVN to TO the DT parts NNS receiving VVG the DT primary JJ impact NN of IN a DT collision NN . SENT I PP Back RB to TO Unibody NP Terms NNS Index NP INDIRECT JJ SECONDARY JJ INERTIAL JJ DAMAGE NN . SENT The DT damage NN to TO the DT opposite JJ end NN of IN a DT vehicle NN from IN which WDT the DT primary JJ damage NN occurred VVD . SENT It PP is VBZ caused VVN by IN the DT inertia NN forces NNS present JJ during IN a DT collision NN . SENT An DT example NN of IN this DT type NN of IN damage NN is VBZ if IN the DT rear JJ end NN of IN a DT car NN is VBZ out RP of IN dimensional JJ tolerance NN as IN the DT result NN of IN a DT front JJ end NN impact NN . SENT This DT type NN of IN damage NN has VHZ often RB been VBN referred VVN to TO as IN Kick NP Up NP or CC Kick NP Down NP . SENT It PP can MD also RB be VB used VVN to TO describe VV the DT cause NN of IN damage NN to TO mechanical JJ components NNS such JJ as IN motor NN mounts VVZ or CC front JJ suspension NN as IN the DT result NN of IN a DT rear JJ end NN collision NN . SENT K NP KINK NN . SENT A DT condition NN to TO a DT structural JJ component NN in IN which WDT the DT metal NN is VBZ folded VVN back RB against IN itself PP through IN direct JJ impact NN or CC through IN compression NN of IN the DT component NN . SENT The DT metal NN is VBZ severely RB weakened VVN and CC if IN repairs NNS are VBP attempted VVN much RB of IN the DT strength NN of IN the DT component NN will MD be VB lost VVN . SENT This DT type NN of IN damage NN normally RB requires VVZ the DT component NN to TO be VB replaced VVN if IN proper JJ strength NN and CC crushability NN are VBP to TO be VB maintained VVN in IN the DT component NN . SENT M NP Back RB to TO Unibody NP Terms NNS Index NP MINIMUM NN OVERLAP VVP SECTIONED VVN PART NN . SENT The DT process NN of IN sectioning VVG a DT structural JJ panel NN such JJ as IN rocker NN panel NN , , pillar NN or CC frame NN rail NN using VVG Tech NP Cor's NP recommended VVD repair NN procedures NNS in IN which WDT the DT panels NNS are VBP slightly RB overlapped VVN and CC welded VVN . SENT P NN PILLAR NN OR CC PANEL NN FORWARD RB BACK RB . SENT A DT condition NN in IN which WDT a DT structural JJ member NN such JJ as IN a DT hinge NN pillar NN is VBZ out RP of IN tolerance NN to TO the DT length NN dimensions NNS . SENT PILLAR NN OR CC PANEL NN HIGH JJ LOW NN . SENT A DT condition NN in IN which WDT a DT structural JJ component NN such JJ as IN a DT hinge NN pillar NN or CC rocker NN panel NN is VBZ out RP of IN tolerance NN to TO the DT datum NN line NN of IN the DT vehicle NN . SENT PILLAR NN OR CC PANEL NN IN IN OUT RB . SENT A DT condition NN in IN which WDT a DT structural JJ component NN such JJ as IN a DT rocker NN panel NN or CC hinge VV pillar NN is VBZ out RP of IN dimensional JJ tolerance NN to TO the DT vehicle NN centerline NN . SENT PILLAR NN TWIST NN . SENT A DT condition NN in IN which WDT a DT hinge NN pillar NN is VBZ out RP of IN square NN from IN the DT inner JJ pillar NN to TO the DT outer JJ pillar NN . SENT The DT pillar NN rolled VVN from IN forces NNS applied VVN to TO the DT hinges NNS or CC outer JJ panels NNS . SENT PULL VV FOR IN ACCESS NN . SENT The DT process NN of IN using VVG some DT type NN of IN pulling VVG equipment NN to TO pull VV a DT damaged JJ part NN of IN a DT vehicle NN out RP so IN repairs NNS can MD be VB performed VVN to TO the DT vehicle NN by IN allowing VVG access NN to TO the DT necessary JJ parts NNS to TO perform VV repairs NNS . SENT An DT example NN of IN this DT may MD be VB if IN a DT fender NN has VHZ jammed VVN a DT hood NN shut VVD , , the DT fender NN will MD need VV to TO be VB pulled VVN prior JJ to TO being VBG able JJ to TO open VV the DT hood NN . SENT R SYM Back RB to TO Unibody NP Terms NNS Index NN RAIL NN HIGH JJ RAIL NN LOW NN . SENT A DT condition NN to TO a DT frame NN rail NN , , apron NN or CC reinforcement NN in IN which WDT the DT dimension NN from IN the DT datum NN line NN to TO the DT measuring VVG point NN is VBZ out RP of IN specification NN . SENT This DT condition NN has VHZ sometimes RB been VBN referred VVN to TO as RB sag VV . SENT RAIL NN SHORT NP . SENT A DT condition NN to TO a DT frame NN rail NN , , apron NN or CC upper JJ reinforcement NN in IN which WDT the DT dimensions NNS of IN the DT vehicle NN are VBP out RP of IN specification NN from IN front NN to TO rear NN of IN the DT vehicle NN . SENT This DT condition NN has VHZ sometimes RB been VBN referred VVN to TO as IN collapse NN , , mash NN and CC crush NN . SENT RESTORE VV CORROSION NN PROTECTION NN . SENT The DT process NN of IN preparing VVG and CC applying VVG corrosion NN resistant JJ materials NNS in IN accordance NN with IN ICAR's NP recommended VVD procedures NNS . SENT RUSTPROOFING NN . SENT The DT application NN of IN an DT aftermarket NN rust NN inhibitor NN , , applied VVN by IN someone NN other JJ than IN the DT automobile NN manufacturer NN , , such JJ as IN the DT dealer NN or CC other JJ vendor NN . SENT S NP SETUP NN . SENT The DT process NN of IN mounting VVG or CC attaching VVG a DT vehicle NN to TO a DT pulling VVG system NN . SENT SIDESWAY NP . SENT A DT condition NN to TO a DT frame NN rail NN , , upper JJ apron NN or CC apron NN reinforcement NN in IN which WDT the DT dimensions NNS from IN the DT vehicle NN centerline NN are VBP out RP of IN specification NN on IN one CD or CC both DT sides NNS . SENT SLEEVE NN SECTION NN . SENT The DT process NN of IN a DT partial JJ structural JJ member NN replacement NN using VVG the DT ICAR NP process NN of IN building VVG and CC installing VVG a DT sleeve NN at IN a DT non JJ factory NN seam NN of IN the DT sectioned VVN component NN . SENT SQUARE JJ AND CC FIT JJ . SENT The DT process NN of IN fitting JJ an DT opening NN for IN proper JJ body NN alignment NN such JJ as IN a DT door NN , , windshield NN , , decklid NN or CC hood NN opening NN . SENT SUPPORT NN FOR IN STRUCTURAL JJ REPLACEMENT NN . SENT The DT process NN of IN supporting VVG a DT vehicle NN in IN the DT correct JJ dimensional JJ tolerance NN while IN crucial JJ structural JJ components NNS are VBP being VBG replaced VVN . SENT This DT includes VVZ parts NNS such JJ as IN inner JJ and CC outer JJ rocker NN panels NNS , , uniside NN assemblies NNS or CC other JJ major JJ components NNS in IN which WDT the DT car NN will MD lose VV its PP$ rigidity NN and CC tend VVP to TO flex VV during IN the DT repair NN process NN . SENT U NP Back RB to TO UnibodyTerms NP Index NP UNDERCOAT NN . SENT The DT process NN of IN spraying VVG a DT tar NN or CC rubber NN based VVN material NN on IN the DT underside NN of IN a DT vehicle NN . SENT This DT may MD be VB done VVN for IN road NN noise NN suppression NN and CC or CC as IN part NN of IN the DT factory NN corrosion NN protection NN or CC as IN part NN of IN an DT aftermarket NN rustproofing NN process NN . SENT Insurance NN Terms NNS A DT B NP C NP D NP E NP G NP H NP I NP M NP N NP O NP P NN S NP T NN U NP W NP Z NP Back RB to TO Top JJ A DT ACCIDENT NN . SENT An DT unforeseeable JJ event NN which WDT may MD produce VV injury NN or CC property NN damage NN . SENT ACCIDENT NN DATE NN . SENT Date NN month NN date NN year NN when WRB the DT accident NN occurred VVD . SENT ACCIDENT NN FREQUENCY NN . SENT A DT method NN of IN measuring VVG the DT safety NN performance NN of IN a DT policyholder NN for IN a DT specified JJ period NN by IN multiplying VVG the DT number NN of IN injuries NNS by IN one CD million CD and CC dividing VVG by IN the DT total JJ number NN of IN workhours NNS worked VVD . SENT or CC when WRB the DT actual JJ workhours NNS are VBP unknown JJ , , the DT measurement NN may MD be VB in IN terms NNS of IN number NN of IN accidents NNS for IN each DT 100 CD , , 000 CD or CC payroll NN . SENT With IN automobile NN policyholders NNS the DT exposure NN may MD be VB either DT number NN of IN miles NNS or CC number NN of IN vehicles NNS . SENT ACCIDENT NN YEAR NN . SENT The DT year NN during IN which WDT an DT accident NN takes VVZ place NN without IN regard NN to TO the DT year NN in IN which WDT it PP is VBZ reported VVN . SENT ACTUAL JJ CASH NN VALUE NN . SENT An DT amount NN equal JJ to TO the DT replacement NN cost NN of IN lost VVN or CC damaged VVN property NN at IN the DT time NN of IN loss NN , , less JJR depreciation NN . SENT ACTUAL JJ DAMAGES NNS . SENT Damage NN that WDT really RB exists VVZ as RB distinguished JJ from IN potential JJ or CC possible JJ damage NN . SENT ACTUARY NN . SENT A DT highly RB specialized JJ mathematician NN professionally RB trained VVN in IN the DT risk NN aspects NNS of IN insurance NN , , whose WP$ functions NNS include VVP the DT calculations NNS involved VVN in IN determining VVG proper JJ insurance NN rates NNS , , evaluating VVG reserves NNS , , and CC in IN various JJ aspects NNS of IN insurance NN research NN . SENT ADJUDICATION NN . SENT The DT process NN of IN deciding VVG whether IN to TO pay VV , , pend VV , , or CC reject VV a DT claim NN based VVN upon IN the DT information NN submitted VVD , , the DT eligibility NN of IN the DT recipient NN , , and CC the DT available JJ benefits NNS . SENT ADJUSTER NN . SENT A DT person NN who WP investigates VVZ and CC settles VVZ losses NNS for IN an DT insurance NN carrier NN . SENT AGENCY NN SYSTEM NN . SENT Insurance NN distribution NN system NN utilizing VVG licensed JJ agents NNS . SENT AGENT NN . SENT Laws NNS of IN all DT states NNS require VVP all DT insurance NN agents NNS to TO be VB licensed VVN by IN the DT state NN to TO sell VV insurance NN . SENT ALL DT RISK NN INSURANCE NN . SENT Property NN and CC liability NN coverage NN for IN all DT perils NNS except IN those DT specifically RB excluded VVN in IN the DT policy NN , , ALTERNATE JJ DISTRIBUTION NN SYSTEM NN . SENT Any DT insurance NN distribution NN system NN that WDT does VVZ not RB utilize VV person NN to TO person NN contact NN . SENT AMOUNT NN OF IN LOSS NN . SENT The DT extent NN of IN loss NN , , expressed VVD monetarily RB . SENT APPRAISAL NN . SENT A DT survey NN by IN an DT impartial JJ expert NN estimating VVG quantity NN , , quality NN or CC value NN of IN property NN to TO determine VV its PP$ insurability NN or CC the DT amount NN of IN loss NN sustained VVD . SENT ARBITRATION NN . SENT Determination NN by IN impartial JJ experts NNS of IN the DT value NN of IN property NN or CC the DT extent NN of IN damage NN . SENT Many JJ insurance NN policies NNS provide VVP for IN appraisals NNS where WRB the DT company NN and CC the DT insured JJ cannot NN agree VVP on IN the DT amount NN or CC the DT extent NN of IN a DT loss NN . SENT ARSON NN . SENT The DT willful JJ and CC malicious JJ burning NN of IN property NN . SENT ASSIGNED VVN RISK NN . SENT A DT risk NN that WDT is VBZ assigned VVN to TO a DT pool NN of IN participating VVG insurers NNS who WP agree VVP to TO accept VV either CC the DT profit NN or CC loss NN associated VVN with IN the DT risk NN . SENT ASSURED VVN . SENT Synonymous JJ with IN insured JJ . SENT One NN who WP has VHZ an DT insurance NN policy NN with IN an DT insurance NN carrier NN . SENT AUTOMOBILE NN DEATH NN INDEMNITY NN COVERAGE NN . SENT Provides VVZ limited JJ life NN insurance NN protection NN to TO insured JJ persons NNS specifically RB named VVN in IN the DT policy NN in IN the DT event NN of IN a DT death NN that WDT is VBZ a DT direct JJ result NN of IN a DT vehicle NN accident NN . SENT Payment NN is VBZ not RB contingent JJ upon IN the DT establishment NN of IN negligence NN , , but CC death NN by IN an DT intentional JJ act NN of IN the DT insured NN is VBZ not RB covered VVN . SENT AUTOMOBILE NN DISABILITY NN INCOME NN COVERAGE NN . SENT Provides VVZ persons NNS specifically RB named VVN in IN the DT policy NN with IN the DT weekly JJ benefit NN shown VVN in IN the DT policy NN in IN the DT event NN of IN continuous JJ total JJ disability NN as IN a DT direct JJ result NN of IN bodily JJ injury NN , , sickness NN , , or CC infection NN caused VVN by IN an DT auto NN accident NN . SENT AUTOMOBILE NN PHYSICAL JJ DAMAGE NN INSURANCE NN . SENT Covers VVZ damage NN or CC loss NN to TO automobile NN of IN policy NN holder NN . SENT AUTOMOTIVE JJ INSURANCE NN , , COMPREHENSIVE JJ . SENT Insurance NN against IN any DT physical JJ loss NN to TO an DT automobile NN except IN by IN collision NN or CC upset JJ . SENT B SYM Back RB to TO InsuranceTerms NP Index NP BASIC JJ POLICY NN . SENT Standard JJ contract NN for IN a DT given VVN policy NN type NN before IN the DT inclusion NN of IN specific JJ riders NNS , , endorsements NNS , , exclusions NNS or CC conditions NNS . SENT BENEFIT NN . SENT Amount NN of IN money NN provided VVN by IN an DT insurance NN policy NN to TO be VB paid VVN for IN losses NNS covered VVN under IN the DT terms NNS of IN the DT policy NN . SENT BENEFIT NN SCHEDULE NN . SENT A DT schedule NN in IN a DT health NN insurance NN policy NN that WDT includes VVZ types NNS of IN services NNS covered VVN by IN the DT policy NN and CC the DT amount NN to TO be VB paid VVN for IN each DT service NN . SENT BINDER NN . SENT A DT written JJ or CC oral JJ contract NN issued VVD temporarily RB to TO place VV insurance NN in IN force NN immediately RB prior RB to TO issuance NN of IN a DT new JJ policy NN or CC endorsement NN of IN an DT existing JJ one CD . SENT A DT binder NN is VBZ subject JJ to TO payment NN of IN the DT premium NN and CC provides VVZ coverage NN under IN the DT terms NNS of IN the DT policy NN to TO be VB issued VVN , , unless IN otherwise RB specified VVN . SENT BLANKET NN COVERAGE NN . SENT A DT Blanket NN form NN is VBZ one CD under IN which WDT property NN is VBZ insured VVN under IN a DT single JJ amount NN applying VVG to TO several JJ different JJ pieces NNS of IN property NN rather RB than IN a DT specific JJ amount NN of IN insurance NN on IN each DT property NN . SENT BODILY JJ INJURY NN BI NP . SENT Injury NN to TO the DT body NN of IN a DT person NN . SENT In IN insurance NN , , also RB refers VVZ to TO the DT coverage NN afforded VVN for IN financial JJ protection NN against IN bodily JJ injury NN of IN a DT person NN resulting VVG from IN an DT accident NN . SENT BROKER NN . SENT One NN who WP is VBZ a DT solicitor NN of IN insurance NN on IN behalf NN of IN his PP$ or CC her PP$ clients NNS . SENT Most JJS states NNS require VVP that IN brokers NNS be VB licensed VVN as IN agents NNS . SENT C SYM Back RB to TO InsuranceTerms NP Index NP CLAIM NN . SENT A DT request NN for IN payment NN for IN a DT loss NN that WDT may MD come VV under IN the DT terms NNS of IN an DT insurance NN contract NN . SENT There EX are VBP two CD types NNS of IN claims NNS . SENT A DT first JJ party NN claim NN is VBZ one CD made VVN by IN the DT policyholder NN for IN reimbursement NN by IN his PP$ or CC her PP$ company NN . SENT A DT third JJ party NN claim NN is VBZ one CD by IN a DT person NN against IN a DT policyholder NN of IN another DT company NN and CC the DT payment NN , , if IN any DT , , will MD be VB made VVN by IN that DT company NN . SENT CLAIMANT NN . SENT One NN who WP makes VVZ a DT claim NN against IN another DT insurance NN company NN . SENT CLAIMS NNS REPRESENTATIVE JJ CR NN . SENT Technical JJ position NN of IN investigating VVG and CC bringing VVG to TO disposition NN minor JJ claims NNS via IN the DT telephone NN . SENT COLLISION NN INSURANCE NN . SENT Insurance NN covering VVG loss NN to TO the DT insured's NNS vehicle NN caused VVN by IN its PP$ collision NN with IN another DT vehicle NN or CC object NN but CC not RB covering VVG personal JJ injury NN or CC property NN damage NN . SENT COMMISSIONER NN OF IN INSURANCE NN . SENT Title NN of IN the DT head NN of IN the DT state NN insurance NN department NN who WP is VBZ responsible JJ for IN the DT enforcement NN of IN insurance NN laws NNS and CC for IN promulgating VVG regulations NNS dealing VVG with IN the DT insurance NN industry NN . SENT COMPREHENSIVE JJ COVERAGE NN . SENT In IN automobile NN insurance NN it PP is VBZ protection NN against IN any DT loss NN or CC damage NN to TO an DT automobile NN except IN by IN collision NN or CC by IN upset NN . SENT In IN other JJ types NNS of IN policies NNS it PP is VBZ insurance NN that WDT covers VVZ under IN one CD insuring VVG agreement NN all DT hazards NNS within IN the DT general JJ scope NN of IN the DT contract NN except IN those DT specifically RB excluded VVN . SENT CONCEALMENT NN . SENT Normally RB means VVZ the DT willful JJ withholding NN of IN material NN fact NN which WDT could MD affect VV an DT insurer's JJ issuance NN of IN a DT policy NN or CC processing NN of IN a DT claim NN . SENT CONDITIONS NNS . SENT Provisions NNS of IN an DT insurance NN policy NN that WDT specify VV CONSERVATION NN . SENT Activities NNS intended VVD to TO keep VV in IN force NN policies NNS from IN lapsing VVG or CC from IN being VBG surrendered VVN . SENT CONTRACT NN . SENT The DT agreement NN between IN an DT insurance NN company NN and CC an DT insured NN . SENT It PP states VVZ the DT legally RB enforceable JJ obligations NNS of IN the DT insurance NN company NN in IN return NN for IN the DT premiums NNS it PP receives VVZ . SENT COVERAGE NN . SENT Specific JJ protection NN provided VVN under IN an DT insurance NN contract NN . SENT D SYM Back RB to TO InsuranceTerms NP Index NP DAMAGE NN . SENT Loss NN or CC harm NN resulting VVG from IN injury NN to TO a DT person NN , , property NN , , or CC to TO one's JJ reputation NN . SENT DAMAGES NNS . SENT The DT monetary JJ amount NN an DT insurance NN company NN is VBZ legally RB obligated VVN to TO pay VV for IN losses NNS incurred VVN . SENT DECLARATION NN . SENT That DT part NN of IN the DT policy NN describing VVG the DT names NNS insured VVN , , address VV , , effective JJ date NN , , term NN of IN the DT policy NN , , applicable JJ coverages NNS , , the DT amount NN of IN insurance NN and CC the DT premium NN . SENT DEDUCTIBLE JJ . SENT A DT dollar NN amount NN , , specified VVN in IN most JJS insurance NN policies NNS , , beyond IN which WDT insurance NN protection NN begins VVZ . SENT The DT insured NN assumes VVZ the DT loss NN up RB to TO the DT limit NN of IN the DT deductible JJ amount NN then RB the DT insurance NN company NN pays VVZ any DT amount NN over IN the DT deductible JJ , , up RB to TO the DT policy NN limit NN . SENT DEPENDENT JJ . SENT One NN who WP relies VVZ on IN another DT for IN economic JJ support NN . SENT In IN insurance NN , , those DT covered VVN under IN the DT policy NN of IN the DT person NN providing VVG that DT support NN . SENT DEPRECIATION NN . SENT A DT decrease NN in IN the DT value NN of IN property NN due JJ to TO age NN , , wear VV and CC tear VV . SENT DISABILITY NN THRESHOLD NN . SENT In IN no DT fault NN auto NN insurance NN states NNS with IN the DT disability NN threshold NN , , it PP provides VVZ that IN a DT victim NN may MD not RB sue VV in IN tort NN unless IN he PP has VHZ been VBN disabled VVN from IN an DT accident NN for IN a DT specific JJ period NN of IN time NN . SENT DOLLAR NN THRESHOLD NN . SENT In IN no DT fault NN auto NN insurance NN states NNS with IN the DT dollar NN threshold NN , , it PP prevents VVZ individuals NNS from IN suing VVG in IN tort NN to TO recover VV for IN pain NN and CC suffering NN unless IN their PP$ medical JJ expenses NNS exceed VVP a DT certain JJ dollar NN amount NN . SENT DOMESTIC JJ CARRIER NN . SENT An DT insurance NN company NN organized VVN in IN a DT given VVN state NN is VBZ referred VVN to TO in IN that DT state NN as IN a DT domestic JJ carrier NN . SENT DRIVE NN IN IN CLAIMS NNS SERVICE NN . SENT Automobile NN insurer's NNS facility NN to TO which WDT an DT insured NN may MD bring VV a DT damaged JJ auto NN in IN order NN to TO facilitate VV the DT adjusting NN of IN claims NNS and CC the DT settlement NN of IN damages NNS . SENT E SYM Back RB to TO InsuranceTerms NP Index NP ENDORSEMENT NN . SENT A DT written JJ amendment NN attached VVN to TO a DT policy NN modifying VVG the DT terms NNS of IN the DT insurance NN contract NN . SENT EXPIRATION NN DATE NN . SENT The DT date NN and CC hour NN on IN which WDT a DT policy NN ceases VVZ to TO protect VV the DT insured NN . SENT F NP FINANCIAL NP RESPONSIBILITY NN LAWS NNS . SENT State NN laws NNS that WDT serve VVP to TO encourage VV , , or CC require VV all DT motorists NNS to TO purchase VV liability NN coverage NN . SENT FLEET NN . SENT Five CD or CC more JJR cars NNS owned VVN by IN one CD insured NN covered VVN under IN one CD automobile NN insurance NN policy NN . SENT FLEET NN POLICY NN . SENT Insurance NN contract NN covering VVG a DT number NN of IN vehicles NNS owned VVN by IN the DT same JJ insured NN . SENT G NP GLASS NN INSURANCE NN . SENT Coverage NN for IN accidental JJ or CC malicious JJ breakage NN or CC chemical NN damage NN to TO glass NN . SENT GRACE NN PERIOD NN . SENT The DT period NN of IN time NN following VVG the DT premium JJ due JJ date NN in IN which WDT the DT premium NN may MD be VB paid VVN . SENT The DT policy NN remains VVZ in IN force NN during IN the DT grace NN period NN . SENT H NP Back RB to TO InsuranceTerms NP Index NP HIRED VVD CAR NN COVERAGE NN . SENT Protection NN for IN insured VVN against IN liability NN incurred VVN while IN using VVG hired VVN automobiles NNS from IN another DT organization NN . SENT I PP INDEPENDENT JJ ADJUSTOR NN . SENT Independent JJ contractor NN for IN hire NN to TO insurance NN companies NNS and CC other JJ organizations NNS to TO investigate VV and CC settle VV claims NNS . SENT INSURANCE NN . SENT The DT contractual JJ relationship NN which WDT exists VVZ when WRB one CD party NN , , in IN consideration NN of IN the DT payment NN of IN a DT premium NN , , agrees VVZ to TO assume VV the DT risk NN of IN loss NN of IN the DT other JJ party NN for IN loss NN caused VVN by IN designated VVN contingencies NNS . SENT INSURANCE NN COMMISSIONER NN . SENT A DT public JJ officer NN of IN a DT state NN or CC other JJ territory NN whose WP$ duty NN it PP is VBZ to TO enforce VV laws NNS applicable JJ to TO insurance NN . SENT INSURANCE NN POLICY NN . SENT A DT contract NN in IN which WDT the DT insurance NN company NN , , for IN a DT designated VVN premium NN , , agrees VVZ to TO pay VV the DT insured NN for IN loss NN covered VVN by IN the DT policy NN when WRB such JJ loss NN occurs VVZ . SENT INSURED VVN . SENT The DT person NN s PP or CC corporation NN whose WP$ insurable JJ interest NN is VBZ protected VVN by IN the DT policy NN . SENT Also RB called VVD Assured VVN . SENT INSURER NN . SENT The DT insurance NN company NN that WDT issues VVZ a DT policy NN to TO a DT policyholder NN . SENT The DT party NN to TO the DT insurance NN contract NN that WDT promises VVZ to TO pay VV losses NNS or CC render VV service NN . SENT L NP Back RB to TO InsuranceTerms NP Index NP LIABILITY NN . SENT Legal JJ obligation NN , , usually RB financial JJ , , for IN a DT loss NN , , debt NN , , penalty NN or CC the DT like IN . SENT LIABILITY NN INSURANCE NN . SENT All DT forms NNS of IN coverage NN which WDT protect VVP an DT insured NN who WP becomes VVZ obligated VVN to TO pay VV because IN of IN bodily JJ injury NN , , property NN damage NN , , or CC other JJ wrongs NNS to TO which WDT the DT insurance NN policy NN applies VVZ . SENT LIABILITY NN LIMITS NNS . SENT The DT sum NN or CC sums NNS beyond IN which WDT a DT liability NN insurance NN company NN does VVZ not RB protect VV the DT insured NN on IN a DT particular JJ policy NN . SENT The DT majority NN of IN policies NNS covering VVG liability NN for IN bodily JJ injury NN have VHP two CD limits NNS . SENT a DT limit NN of IN liability NN to TO any DT one CD person NN and CC , , subject JJ to TO the DT personal JJ limit NN , , another DT and CC usually RB higher JJR limit NN for IN any DT single JJ accident NN where WRB more JJR than IN one CD person NN in IN involved VVN . SENT LIEN NN . SENT A DT claim NN on IN another's JJ property NN as IN a DT security NN for IN a DT debt NN or CC charge NN . SENT LIFETIME NN MAXIMUM NN . SENT The DT maximum JJ amount NN that IN major JJ medical JJ will MD pay VV toward IN an DT insured's NN claims VVZ in IN a DT lifetime NN . SENT LOSS NN . SENT Value NN reduction NN in IN an DT insured's JJ property NN caused VVN by IN an DT insured JJ peril NN . SENT Amount NN sought VVD in IN a DT claim NN . SENT Amount NN paid VVD on IN behalf NN of IN an DT insured NN under IN an DT insurance NN contract NN . SENT M NP Back RB to TO InsuranceTerms NP Index NP McCARRAN NP FERGUSON NP ACT NN . SENT 1945 CD Federal NP legislation NN in IN which WDT the DT Congress NP declared VVD that IN the DT states NNS may MD continue VV to TO regulate VV the DT insurance NN industry NN . SENT MECHANIC'S NP LIEN NN . SENT Protection NN given VVN to TO laborers NNS and CC suppliers NNS in IN the DT form NN of IN a DT lien NN on IN the DT property NN that WDT has VHZ been VBN improved VVN or CC repaired VVN . SENT N NP NEGLIGENCE NN . SENT Failure NN to TO do VV the DT correct JJ and CC prudent JJ thing NN , , whether IN by IN omission NN or CC commission NN , , in IN a DT particular JJ situation NN . SENT NET JJ LOSS NN . SENT The DT amount NN of IN loss NN sustained VVN by IN an DT insurer NN after IN deducting VVG all DT applicable JJ reinsurance NN , , salvage NN and CC subrogation NN recoveries NNS . SENT NO DT FAULT NN INSURANCE NN . SENT Permits VVZ automobile NN accident NN victims NNS to TO be VB directly RB reimbursed VVN for IN medical JJ and CC hospital NN expenses NNS and CC loss NN of IN income NN by IN their PP$ own JJ insurance NN company NN regardless RB of IN who WP was VBD at IN fault NN . SENT Massachusetts NP included VVD property NN damage NN . SENT NOTICE NN OF IN LOSS NN . SENT Notification NN to TO an DT insurance NN company NN by IN an DT insured NN or CC claimant NN that IN a DT loss NN has VHZ occurred VVN . SENT Written JJ notice NN may MD be VB required VVN , , although IN many JJ companies NNS accept VVP notice NN by IN telephone NN . SENT O NP Back RB to TO InsuranceTerms NP Index NP OCCUPATIONAL JJ SAFETY NN AND CC HEALTH NN ACT NN . SENT 1970 CD legislation NN that WDT set VVD Federal JJ standards NNS for IN work NN place NN safety NN and CC imposed VVN fines NNS for IN failure NN to TO meet VV them PP . SENT OMNIBUS JJ CLAUSE NN . SENT Policy NN extending VVG coverage NN to TO others NNS using VVG a DT particular JJ automobile NN without IN specifically RB naming VVG them PP in IN the DT policy NN . SENT OPEN JJ . SENT The DT status NN of IN a DT claim NN that WDT is VBZ pending VVG settlement NN . SENT P NN PARTIAL JJ LOSS NN . SENT A DT loss NN , , covered VVN under IN an DT insurance NN policy NN , , which WDT does VVZ not RB completely RB destroy VV the DT property NN . SENT PARTY NN . SENT An DT individual JJ or CC other JJ legal JJ entity NN who WP enters VVZ into IN a DT contract NN or CC other JJ legal JJ proceeding NN . SENT POLICY NN . SENT A DT printed JJ document NN issued VVN to TO the DT insured NN by IN the DT company NN stating VVG the DT terms NNS of IN the DT insurance NN contract NN . SENT POLICY NN TERMS NNS . SENT The DT length NN of IN time NN an DT insurance NN policy NN is VBZ in IN force NN , , contingent JJ upon IN payment NN of IN contractual JJ premiums NNS . SENT POLICY NN YEAR NN . SENT The DT 365 CD or CC 366 CD days NNS between IN annual JJ premium NN dates NNS . SENT the DT year NN commencing VVG with IN the DT effective JJ date NN of IN the DT policy NN or CC with IN an DT anniversary NN of IN that DT date NN . SENT POLICYHOLDER NN . SENT The DT individual NN or CC organization NN in IN whose WP$ name NN a DT policy NN is VBZ written VVN . SENT synonymous JJ with IN Insured JJ , , Assured JJ or CC Risk NN . SENT PRE NP ACCIDENT NN CONDITION NN . SENT Condition NN of IN vehicle NN prior RB to TO the DT accident NN PREMIUM NN . SENT The DT amount NN of IN money NN charged VVD a DT policyholder NN for IN an DT insurance NN policy NN . SENT PREMIUM NN RATE NN . SENT The DT price NN per IN unit NN of IN insurance NN . SENT PRINCIPAL NN . SENT In IN suretyship NN , , the DT party NN whose WP$ honesty NN or CC performance NN is VBZ guaranteed VVN . SENT PROOF NN OF IN LOSS NN . SENT Policy NN owner's NNS formal JJ report NN of IN a DT loss NN , , containing VVG information NN so IN the DT insurer NN can MD determine VV the DT extent NN of IN its PP$ liability NN . SENT S PP Back RB to TO InsuranceTerms NP Index NP SALVAGE NN . SENT Proceeds NNS of IN sold VVN property NN secured VVN after IN the DT loss NN to TO reduce VV the DT loss NN sustained VVD , , such JJ as IN the DT sale NN of IN a DT totaled VVN automobile NN . SENT SELECTION NN OF IN RISK NN . SENT The DT process NN of IN identifying VVG and CC classifying VVG the DT potential JJ degree NN of IN risk NN represented VVN by IN a DT proposed VVN insured NN . SENT T NN TORT NN . SENT In IN general JJ a DT civil JJ wrong JJ , , other JJ than IN breach NN of IN contract NN , , for IN which WDT a DT court NN will MD provide VV a DT remedy NN in IN the DT form NN of IN a DT suit NN for IN damages NNS . SENT TORT NN SYSTEM NN . SENT Legal JJ system NN providing VVG that DT civil JJ action NN can MD be VB brought VVN to TO redress VV wrongful JJ injury NN or CC damage NN . SENT TOTAL JJ LOSS NN . SENT Loss NN to TO the DT insured NN of IN the DT entire JJ value NN of IN goods NNS or CC other JJ property NN insured VVN , , or CC a DT loss NN entailing VVG the DT payment NN of IN the DT full JJ face NN amount NN of IN an DT insurance NN contract NN . SENT TOWING VVG . SENT Insures VVZ against IN charges NNS for IN towing VVG and CC road NN service NN at IN the DT place NN of IN disablement NN , , with IN a DT maximum JJ amount NN stipulated VVD for IN each DT occurrence NN . SENT U NP Back RB to TO InsuranceTerms NP Index NP UMPIRE NN . SENT An DT impartial JJ third JJ party NN selected VVN in IN an DT arbitration NN to TO make VV a DT decision NN . SENT Any DT decision NN made VVN by IN two CD of IN the DT three CD people NNS is VBZ binding VVG . SENT UMPIRE NN CLAUSE NN . SENT Part NN of IN some DT insurance NN contracts NNS providing VVG that IN in IN the DT event NN of IN an DT individual NN or CC company NN filing VVG a DT claim NN and CC the DT insuring VVG company NN cannot NN agree VVP on IN the DT settlement NN of IN a DT loss NN , , each DT party NN may MD select VV an DT arbitrator NN and CC the DT two CD arbitrators NNS select VVP an DT umpire NN . SENT The DT insured NN and CC the DT insurance NN company NN agree VVP to TO abide VV by IN the DT decision NN of IN the DT majority NN vote NN of IN the DT arbitrators NNS and CC umpire NN . SENT UNDERINSURED JJ MOTORIST NN COVERAGE NN . SENT Coverage NN is VBZ intended VVN to TO cover VV you PP and CC passengers NNS in IN your PP$ car NN for IN losses NNS unpaid JJ because IN sufficient JJ bodily JJ liability NN limits NNS are VBP not RB available JJ from IN the DT policy NN of IN an DT at IN fault NN driver NN . SENT How WRB and CC under IN what WP circumstances NNS the DT coverage NN becomes VVZ operative NN varies VVZ in IN different JJ states NNS . SENT UNDERWRITER NN . SENT Person NN who WP studies VVZ risks NNS , , determines VVZ rates NNS and CC coverages NNS , , and CC decides VVZ if IN the DT risk NN is VBZ acceptable JJ . SENT UNDERWRITING NN . SENT A DT process NN which WDT evaluates VVZ an DT applicant NN against IN pre NP established VVD criteria NNS for IN insurability NN to TO determine VV whether IN the DT applicant NN will MD be VB rejected VVN or CC accepted VVN for IN coverage NN and CC whether IN at IN standard JJ or CC modified JJ rates NNS . SENT W NP Back RB to TO InsuranceTerms NP Index NP WARRANTY NN . SENT Promises NNS made VVN by IN the DT insured NN , , which WDT if IN not RB kept VVN or CC untrue JJ , , will MD void VV the DT policy NN . SENT Y NP YOUTHFUL JJ INSURED NN . SENT An DT insured JJ male NN or CC female JJ under IN 25 CD years NNS of IN age NN . SENT Z SYM ZONE NN EXAMINATIONS NNS . SENT Triennial JJ examination NN of IN insurance NN companies NNS as RB established VVN by IN the DT National NP Association NP of IN Insurance NP Commissioners NNS . SENT Computer NN Estimating VVG Terms NNS C NP D NP F NP I NP K NP L NP M NP N NP O NP P NN R NP S NP T NN U NP W NP Back RB to TO Top JJ C NP CADDY NN . SENT The DT case NN that WDT holds VVZ your PP$ CD NN inside IN the DT drive NN mechanism NN . SENT All DT drives NNS do VVP not RB require VV a DT caddy NN , , and CC those DT that WDT do VVP usually RB come VV with IN one CD CD NN caddy NN . SENT CD NP ROM NP . SENT An DT acronym NN for IN Compact JJ Disk NN Read VV Only RB Memory NP . SENT A DT special JJ optical JJ storage NN device NN that WDT can MD contain VV millions NNS of IN bytes NNS of IN information NN . SENT You PP cannot NN save VV or CC write VV to TO Read VV Only JJ CD NN . SENT CERTIFICATION NN CODE NN CRT NP . SENT Appearing VVG on IN the DT Parts NP Exchange NP New NP Locate VVP Report NP , , this DT code NN indicates VVZ a DT part NN is VBZ certified VVN by IN CAPA NP Certified NP Aftermarket NN Parts NP Association NP . SENT CLASSIFICATION NN CODE NN CLS NP COLLISION NN . SENT A DT type NN of IN Loss NN if IN damage NN to TO an DT insured JJ vehicle NN results NNS from IN impact NN with IN another DT vehicle NN or CC object NN . SENT Usually RB abbreviated VVN as IN COLL NP or CC COL NN . SENT COMPREHENSIVE JJ . SENT A DT type NN of IN Loss NN if IN damage NN to TO an DT insured JJ vehicle NN results NNS from IN something NN other JJ than IN collision NN e NN . SENT g NN . SENT fire NN , , hailstorm NN or CC vandalism NN . SENT COMPUTER NN GRAPHICS NNS . SENT Pictorial JJ representations NNS such JJ as IN diagrams NNS , , drawings NNS , , or CC charts NNS generated VVN on IN a DT computer NN . SENT CONFIGURATION NN . SENT The DT specific JJ combination NN of IN hardware NN and CC software NN being VBG utilized VVN in IN a DT personal JJ computer NN application NN , , or CC the DT selected VVN parameters NNS that WDT determine VVP the DT operation NN of IN a DT device NN . SENT CONTROL NN ENTRY NN . SENT Any DT Damage NN Entry NN in IN an DT Audatex NP Estimate NP that WDT contains VVZ a DT Guide NP Number NP . SENT CONTROL NN LOG NN NUMBER NN . SENT In IN the DT Audatex NP system NN , , the DT log NN number NN assigned VVN to TO the DT transaction NN used VVN to TO initiate VV the DT original JJ Estimate NP or CC Schedule NN is VBZ the DT Control NP Log NN Number NP . SENT CORRECTION NN UPDATE NN . SENT In IN the DT Audatex NP system NN , , the DT log NN number NN assigned VVN to TO the DT transaction NN used VVN to TO initiate VV the DT original JJ Estimate NP or CC Schedule NN is VBZ the DT Control NP Log NN Number NP . SENT CPU NN . SENT An DT acronym NN for IN Central NP Processing NP Unit NP . SENT Another DT term NN for IN a DT computer's NP microprocessor NN i NP . SENT e SYM . SENT the DT control NN center NN of IN the DT computer NN where WRB all DT calculations NNS take VVP place NN . SENT CURSOR NN . SENT Blinking VVG rectangle NN or CC other JJ graphic JJ symbol NN indicating VVG where WRB the DT next JJ keyboard NN input NN will MD be VB placed VVN . SENT D SYM Back RB to TO Computer NP Estimating VVG Terms NNS Index NP DATA NNS BASE NN . SENT Integrated JJ file NN of IN information NN organized VVN for IN access NN and CC retrieval NN . SENT DATA NN TRANSMISSION NN . SENT A DT communications NNS event NN where WRB data NN is VBZ transmitted VVN from IN one CD device NN to TO another DT . SENT DEDICATED JJ LINE NN . SENT A DT telephone NN line NN used VVN for IN the DT sole JJ purpose NN of IN data NN transmission NN via IN a DT computer NN . SENT DEFAULT NN . SENT The DT standard JJ choice NN , , option NN or CC selection NN automatically RB used VVN by IN a DT computer NN program NN unless IN changed VVN by IN the DT user NN . SENT DIAGNOSTICS NNS . SENT A DT specific JJ software NN or CC hardware NN procedure NN designed VVN to TO verify VV a DT computer's JJ operation NN and CC identify VV reasons NNS for IN failure NN . SENT DISK NN . SENT The DT magnetic JJ medium NN on IN which WDT the DT computer NN stores NNS information NN . SENT The DT disk NN can MD be VB a DT floppy JJ disk NN or CC a DT hard JJ disk NN . SENT DISK NN DRIVE NN . SENT The DT mechanism NN that WDT rotates VVZ a DT disk NN past IN the DT read NN write VV device NN or CC head NN inside IN a DT CPU NN . SENT DOWNLOAD NP . SENT A DT method NN of IN data NN transmission NN whereby WRB a DT computer NN receives VVZ data NNS from IN another DT device NN i NP . SENT e SYM . SENT a DT host NN or CC personal JJ computer NN . SENT DRIVER NN . SENT Specific JJ software NN that WDT enables VVZ and CC controls VVZ the DT interaction NN of IN a DT device NN e NN . SENT g NN . SENT a DT printer NN with IN a DT computer NN program NN . SENT F SYM Back RB to TO Computer NP Estimating VVG Terms NNS Index NP FACTORY NN PROVIDED VVD . SENT All DT standard JJ and CC optional JJ vehicle NN parts NNS installed VVN at IN the DT factory NN by IN the DT original JJ manufacturer NN of IN the DT vehicle NN . SENT FIELD NN INSPECTION NN . SENT An DT inspection NN where WRB the DT estimator NN FILE NN . SENT A DT collection NN of IN information NN stored VVN on IN a DT disk NN e NN . SENT g NN . SENT document NN , , a DT system NN file NN , , or CC an DT application NN . SENT H NP HARDWARE NN . SENT The DT physical JJ components NNS of IN a DT system NN i NP . SENT e SYM . SENT mechanical JJ or CC electrical JJ . SENT I PP INCLUDED VVD OPERATION NN . SENT Any DT operation NN e NN . SENT g NN . SENT removal NN and CC replacement NN of IN a DT part NN completed VVN in IN its PP$ entirety NN while IN performing VVG another DT separate JJ operation NN . SENT INSURED VVN . SENT The DT person NN purchasing VVG the DT insurance NN policy NN from IN the DT insurance NN company NN . SENT INTERFACE NN . SENT Boundary NN where WRB two CD or CC more JJR devices NNS interact VV , , or CC a DT program NN enabling VVG separate JJ elements NNS to TO work VV together RB . SENT K NP Back RB to TO Computer NP Estimating VVG Terms NNS Index NP K NP . SENT Abbreviation NN for IN kilobyte NN in IN relation NN to TO computers NNS . SENT represents VVZ 1 CD , , 000 CD bytes NNS . SENT L NP LABOR NN RATE NN . SENT The DT dollar NN amount NN applied VVN to TO flat JJ rate NN labor NN time NN specifically RB quoted VVN in IN dollars NNS per IN hour NN by IN labor NN category NN frame NN . SENT mechanical JJ electrical JJ . SENT refinish NNS . SENT sheetmetal JJ . SENT LIABILITY NN . SENT A DT type NN of IN Loss NN resulting VVG from IN damage NN or CC injury NN one NN individual NN causes VVZ to TO another DT for IN which WDT the DT first JJ individual NN is VBZ legally RB liable JJ . SENT Abbreviated VVN LIAB NP . SENT LOG VV ON RP , , LOG VV OFF RP . SENT Typing VVG a DT password NN or CC designated VVN work NN before IN starting VVG to TO use VV an DT application NN and CC typing VVG another DT to TO indicate VV when WRB you PP are VBP finished VVN . SENT M NP Back RB to TO Computer NP Estimating VVG Terms NNS Index NP MANUAL JJ ENTRY NN . SENT A DT damage NN entry NN for IN a DT part NN or CC operation NN that WDT is VBZ not RB assigned VVN a DT guide NN number NN . SENT MEMORY NN . SENT The DT place NN in IN the DT computer NN that WDT temporarily RB stores VVZ information NN while IN you PP are VBP working VVG with IN it PP . SENT MENU NN . SENT A DT list NN of IN options NNS or CC commands NNS in IN a DT computer NN program NN visible JJ on IN the DT screen NN . SENT MENU NN BAR NN . SENT The DT horizontal JJ strip NN at IN the DT top NN of IN the DT screen NN that WDT contains VVZ menu NN titles NNS . SENT MICROCOMPUTER JJR . SENT Personal JJ computer NN containing VVG processor NN , , input NN and CC display NN devices NNS , , and CC memory NN . SENT MICROPROCESSOR NN . SENT The DT computer's JJ main JJ brain NN , , the DT control NN center NN for IN the DT computer NN . SENT This DT lets VVZ computers NNS communicate VV over IN the DT existing JJ phone NN lines NNS . SENT MODEM NN . SENT A DT device NN that WDT takes VVZ electronic JJ information NN from IN a DT computer NN and CC converts VVZ it PP into IN sounds NNS that WDT can MD be VB transmitted VVN over IN phone NN lines NNS . SENT This DT lets VVZ computers NNS communicate VV over IN the DT existing JJ phone NN lines NNS . SENT MULTI NNS LEVEL NN ASSEMBLY NN . SENT The DT combination NN of IN two CD or CC more JJR assemblies NNS , , plus CC related JJ component NN parts NNS , , that WDT are VBP sold VVN by IN the DT manufacturer NN under IN one CD part NN number NN . SENT N NP Back RB to TO Computer NP Estimating VVG Terms NNS Index NP NAGS NNS NATIONAL NP AUTO NN GLASS NN SPECIFICATION NN , , INC NP . SENT . SENT An DT organization NN that WDT specifies VVZ , , certifies VVZ , , and CC publishes VVZ pricing NN for IN automotive JJ glass NN . SENT NON JJ OEM NP . SENT All DT parts NNS that WDT are VBP considered VVN Aftermarket NN , , Economy NP , , and CC Salvage NP that WDT are VBP not RB made VVN by IN the DT original JJ manufacturer NN . SENT O NP OEM NP ORIGINAL JJ EQUIPMENT NN MANUFACTURER NN . SENT A DT new JJ replacement NN part NN or CC accessory JJ that IN is VBZ manufactured VVN by IN and CC available JJ through IN the DT vehicle NN manufacturer's NN parts NNS distribution NN network NN . SENT ON IN LINE NN . SENT To TO be VB on IN and CC ready JJ to TO go VV . SENT For IN example NN , , when WRB a DT printer NN is VBZ on IN line NN , , it's NNS turned VVD on IN , , contains VVZ paper NN , , and CC is VBZ all RB ready JJ to TO print VV . SENT ORIGINAL JJ PRICE NN . SENT The DT part NN price NN effective JJ on IN the DT date NN that IN an DT estimate NN was VBD originally RB processed VVN . SENT OVERHAUL NN . SENT A DT type NN of IN flat JJ rate NN labor NN that WDT contains VVZ R NP I NP and CC R NP R NP labor NN plus CC time NN to TO completely RB disassemble VV and CC re IN assemble VV an DT assembly NN e NN . SENT g NN . SENT bumpers NNS , , suspension NN , , drive NN axles NNS , , and CC steering NN . SENT P NN Back RB to TO Computer NP Estimating VVG Terms NNS Index NP PAINT NN MATERIAL NN . SENT The DT cost NN for IN paint NN and CC materials NNS is VBZ calculated VVN by IN multiplying VVG the DT value NN entered VVN in IN Rate NP 5 CD of IN the DT Audatex NP Rates NP Calculations NNS screen NN by IN the DT total JJ number NN of IN net JJ labor NN . SENT PARTIAL JJ REPLACE VVP OPERATION NN . SENT The DT partial JJ replacement NN of IN a DT service NN part NN e NN . SENT g NN . SENT quarter NN panel NN belt NN cut NN , , molding NN kit NN , , etc FW . SENT PASSWORD NN . SENT Required VVN code NN permitting VVG an DT individual JJ estimate NN preparer's NNS entry NN into IN protected JJ parts NNS of IN a DT program NN . SENT PERIPHERALS NNS . SENT Any DT item NN attached VVN to TO the DT outside NN of IN the DT computer NN such JJ as IN a DT printer NN , , modem NN , , monitor VV , , or CC keyboard NN . SENT PORT NN . SENT A DT connection NN on IN the DT back NN of IN a DT computer NN to TO which WDT are VBP attached VVN various JJ peripherals NNS . SENT The DT two CD primary JJ ports NNS are VBP the DT serial JJ port NN and CC the DT printer NN port NN , , although IN the DT keyboard NN and CC monitor NN connections NNS can MD also RB be VB called VVN ports NNS . SENT PRELOAD NP . SENT A DT feature NN that WDT allows VVZ the DT estimate NN preparer NN to TO create VV reusable JJ files NNS with IN data NNS common JJ to TO many JJ estimates NNS e NN . SENT g NN . SENT remarks NNS , , labor NN rates NNS , , etc FW . SENT . SENT PRIMARY JJ IMPACT NN . SENT Indicates VVZ the DT area NN of IN the DT Loss NN vehicle NN that WDT sustained VVD the DT most RBS severe JJ damage NN . SENT PRINTOUT NN . SENT Printed VVN output NN from IN a DT computer NN . SENT PROGRAM NN . SENT A DT special JJ file NN on IN disk NN that WDT contains VVZ instructions NNS for IN the DT computer NN . SENT PROMPT VV . SENT A DT symbol NN i NP . SENT e SYM . SENT c LS . SENT or CC a DT field NN where WRB a DT command NN is VBZ given VVN , , information NN is VBZ entered VVN or CC a DT choice NN i NP . SENT e SYM . SENT Y NP N NP is VBZ made VVN . SENT R SYM Back RB to TO Computer NP Estimating VVG Terms NNS Index NP R NP I PP REMOVE VV AND CC INSTALL VV . SENT Refers VVZ to TO a DT flat JJ rate NN labor NN for IN the DT removal NN and CC reinstallation NN of IN the DT same JJ part NN or CC assembly NN generally RB to TO gain VV access NN to TO another DT part NN . SENT RAG NN RULE NN . SENT Because IN the DT Radiator NN , , Air NP conditioning NN condenser NN , , and CC Gas NP tank NN usually RB require VVP removal NN from IN a DT vehicle NN when WRB they PP are VBP repaired VVN , , the DT automatic JJ addition NN of IN the DT necessary JJ R NN I NN labor NN . SENT RAM NN . SENT Random NP Access NP Memory NP , , the DT primary JJ type NN of IN memory NN storage NN in IN a DT PC NN that IN stores NNS information NN temporarily RB while IN you PP are VBP working VVG on IN it PP . SENT Information NN in IN RAM NN is VBZ temporary JJ . SENT It's NNS gone VVN forever RB if IN you PP turn VVP the DT power NN off RP without IN saving NN . SENT RATES NNS . SENT The DT percentage NN or CC dollar NN amounts NNS applied VVN to TO labor NN , , labor NN tax NN and CC parts NNS tax NN . SENT RELATED VVN PRIOR JJ DAMAGE NN . SENT Damage NN to TO the DT vehicle NN that WDT occurred VVD prior RB to TO the DT current JJ loss NN . SENT When WRB prior JJ damage NN exists VVZ , , the DT estimator NN determines VVZ an DT amount NN to TO be VB deducted VVN from IN the DT cost NN to TO repair VV or CC replace VV the DT damaged JJ part NN since IN the DT part NN was VBD not RB in IN original JJ condition NN when WRB the DT current JJ loss NN occurred VVD . SENT ROM NP . SENT Read VV Only RB Memory NP , , the DT part NN of IN memory NN that WDT contains VVZ information NN or CC instructions NNS , , Information NN in IN ROM NP cannot NN be VB changed VVN as IN it PP is VBZ Read VV Only RB . SENT S PP Back RB to TO Computer NP Estimating VVG Terms NNS Index NP SCROLL NN . SENT To TO move VV what WP is VBZ displayed VVN on IN a DT computer's JJ screen NN e NN . SENT g NN . SENT a DT list NN , , a DT document NN so RB that IN a DT different JJ part NN of IN it PP is VBZ visible JJ . SENT This DT can MD be VB done VVN by IN using VVG the DT page NN up RP and CC page NN down IN keys NNS . SENT SOFTWARE NN . SENT Programs NNS or CC programs NNS containing VVG instructions NNS that WDT control VVP computer NN hardware NN . SENT SUPPLIER NN CODE NN SPL NP CDE NP . SENT A DT numeric JJ code NN i NP . SENT e SYM . SENT 01 CD , , 02 CD , , 03 CD etc NN . SENT identifying VVG the DT supplier NN s PP of IN each DT individual JJ part NN . SENT The DT supplier NN code NN is VBZ helpful JJ when WRB multiple JJ suppliers NNS are VBP listed VVN on IN the DT report NN . SENT T NN TRANSMIT VV . SENT To TO send VV a DT transaction NN to TO another DT system NN by IN way NN of IN a DT modem NN . SENT TWO CD STAGE NN PAINT NN . SENT The DT application NN of IN a DT clear JJ coat NN of IN paint NN over IN a DT base JJ color NN coat NN of IN paint NN on IN an DT automobile NN . SENT U NP Back RB to TO Computer NP Estimating VVG Terms NNS Index NP UNRELATED JJ PRIOR JJ DAMAGE NN . SENT Damage NN to TO a DT part NN of IN the DT loss NN , , vehicle NN that WDT was VBD present JJ prior RB to TO the DT current JJ loss NN . SENT UPLOAD NP . SENT A DT method NN of IN data NN transmission NN whereby WRB a DT computer NN sends VVZ data NNS to TO another DT device NN i NP . SENT e SYM . SENT a DT host NN or CC personal JJ computer NN . SENT V NN VIN NP . SENT The DT vehicle NN identification NN number NN assigned VVN to TO each DT automobile NN by IN its PP$ manufacturer NN to TO identify VV the DT model NN , , year NN , , production NN sequence NN and CC other JJ vehicle NN specific JJ information NN . SENT W NP WRITE VVP PROTECT VV . SENT The DT tab NN setting VVG on IN a DT diskette NN that WDT makes VVZ it PP impossible JJ to TO alter VV data NNS . SENT A DT 3 CD . SENT 5 CD diskette NN is VBZ write VV protected VVN when WRB you PP can MD see VV through IN the DT little JJ hole NN in IN the DT upper JJ right NN corner NN . SENT Time NN Terms NNS Back RB to TO Top JJ ACTUAL JJ TIME NN . SENT Only JJ time NN spent VVN on IN the DT job NN . SENT AVAILABLE JJ HOURS NNS . SENT Number NN of IN productive JJ employees NNS x SYM 7 CD . SENT 5 CD hours NNS BILLED VVD HOURS NNS . SENT Number NN of IN hours NNS billed VVN that IN day NN per IN specified JJ period NN i NP . SENT e SYM . SENT day NN , , week NN , , month NN COMMISSION NN PAY NN . SENT A DT percentage NN of IN the DT total JJ labor NN billed VVD paid VVN to TO technician NN for IN the DT work NN done VVN FLAT JJ RATE NN . SENT Not RB time NN but CC work NN units NNS as RB in IN bid NN time NN FLAT JJ RATE NN PAY NN . SENT An DT amount NN of IN money NN per IN hour NN produced VVD HOURLY JJ PAY NN . SENT Amount NN paid VVD to TO the DT technician NN per IN hour NN regardless RB how WRB much RB is VBZ produced VVN PRODUCTIVE JJ TIME NN . SENT Billed VVN hours NNS divided VVN by IN available JJ hours NNS